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△ Android 7.1.2
△ HDMI 2.0
△ Low Cost
△ Personalized User Interface (Hotel/Hospital/Community…)
△ Advertisement System (ADS) Imbedded
 Product overview	
The FMUSER IPTV HD STB is an Android 7.1-based set-top box with 4K H.265/HEVC decoding and HDMI 2.0 output. It processes IPTV streams via 10/100M Ethernet or dual-band Wi-Fi, supporting Widevine L1 DRM and custom EPG interfaces. The compact device integrates ad systems and runs commercial apps, ideal for hospitality TV systems and community IPTV deployments.
Key feature
Android 7.1 flexibility: Supports Netflix, Skype, and third-party apps via Google Play
Specifications
	Hardware
 
	CPU
	RK3229, 28nm Quad core Cortex A7, High cost performance 4K OTT Box solution

	
	GPU
	ARM Mali-400 GPU

	
	HDMI
	Including an HDMI 2.0 for HDMI 2.0 for 4K YUV420@60Hz with HDCP 1.4/2.2

	
	
	Support 4K 10-bit H.265/H.264/VP9 video playback and display

	
	Memory
	1GB DDRIII 

	
	Flash
	8GB Nand Flash

	
	WiFi
	2.4G，802.11 b/g/n,

	
	Wired network
	Ethernet GMAC 10/100/100M Ethernet controller

	
	
	Support 10/100/1000 data transfer rate and RGMII interface

	
	
	Support 10/100Mbps data transfer rate and RGMII interface

	
	IR
	Infra Remote control

	
	Power Supply
	DC input  5V/2A

	Software
 
	OS
	Android 7.1

	
	3D
	Hardward 3D graphics acceleration 

	
	Video decoding
	4K VP9 Video decoder, 4K 10-bits H.265/H.264 video decoder

	
	
	1080P other video decoders (VC-1, MPEG-1/2/4, VP6/8)

	
	
	Support conversion from BT.2020 to Rec.709/Rec.601

	
	
	Video post processor: de-interlace

	
	
	H.263/H.264 2160P@ 24fps
VC-1 ,MPEG - 1 1080p @ 60fps
MPEG- 2 2160P @ 24fps
MPEG-4 1080P @ 60fps
AVS 1080p @ 60fps
 MVC 2160P @ 24fps
WMV,3GP,MKV,ASF,3G2M4V,MJPEG,RV8,RV9,RV10 1080P@60fps

	
	
	Support HEVC decoder

	
	
	Support Main/Main10 HEVC/H.265 decoder, 4K @ 60FPS

	
	
	Support 4096x2304 resolution

	
	
	Support HDMI 720P-2160P FUII 3D HD( 2160P, 3840 * 2160 ), 4K+2 K

	
	
	Support flash11.1

	
	Video Decoder format
	H.264,H.265,VP8,MVC(1080P)

	
	Video format
	Supports DIVD/DIVX/REAL8 / 9 / 10, RV, RM, RMVB, PMP, FLV, MP4, M4V, VOB, VP6, VP8 2160P @ 24fps 

	
	Audio format
	Supports MP1, MP2, MP3, WMA, OGG, AAC, M4A , FLAC, APE,  AMR, RA, WAV, etc

	
	Picture format
	Supports JPG, JPEG, BMP, GIF, PNG, JFIF etc Resolution 8192x8192

	
	HDD file system
	FAT16 / FAT32 / NTFS

	
	Support Subtitle
	SRT, SMI, SUB, SSA, IDX+USB

	
	XBMC/KODI
	Support

	
	DRM
	Widewine Level1, DRM PlayReady ,Verimatrix, built in Trustzone,
HDCP 2.2/1.4

	
	Support language
	Chinese, English, Germany, Japanese, Korea etc.  multilateral languages

	Stream In/Out
	1*HDMI 2.0
	Built-in HDMI 2.0 transmitter including both controller and PHY with CEC and HDCP, 4K @ 60FPS max resolution output

	
	1* SD Card
	to 64GB

	
	4*USB HOST
	2High speed USB 2.0,support USB DISK and USB HDD

	
	1*SPDIF
	SPDIF output

	
	1*RJ45
	Ethernet:10/100M, standard RJ-45

	
	1*Power input
	5V/2A

	
	Accessories
	Gift box
Power charger adapter 
HDMI cable (optional)
IR remote control  (optional)
User's Manual

	Applications
	Online
	Browse all video websites, support Netflix, Hulu, Flixster, youtube etc

	
	Apps
	Apps download freely form android market, amazon appstore etc

	
	Medium
	Local Media playback, support HDD, U disck ,SD card

	
	Talk online
	Support SKYPE video call, MSN, facebook, twitter, QQ  etc

	
	Others
	Support WiFi hotpiont, could  be as a wireless router
Support DLNA, Google TV Remote, LAN, 3D Moive, Email, office suit etc

	Packing
	Dimension
	118*118*25 mm

	
	Approx weight 
	400g


 
System Construction
[image: IMG_257]
[image: IMG_258]
Advantages
Personalized EPG Interface
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* Personalized EPG interface for hotel, hospital, Community and other industries. 
* System wallpaper is changeable and EPG content is editable.
* Various business modes blend in IPTV system
* Support modular interface and convenient to docking with third part manage software
 
Advertisement System—Value added Services
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* Hotel, hospital and community version can support set up advertisement business to increase revenues.
* Ad modes include booting ad, Menu ad (only for hospital and community version), VOD ad, pictures and text ad etc.
Mass HD Programs

* 1080P/60Hz full HD video
* Mass resource of Video on Demand including movies, entertainments, factual shows and etc
* Live programs synchronized broadcast
 
Strength and After-sale Services
* FMUSER IPTV system is with solid quality based on FMUSER’s own DTV head-end equipment
* The whole system is self research and developed, which makes it easy for the after-sale maintenances
* Skilled after-sale supporting team
 
 
·  


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.

   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image4.jpeg
Live/VOD programs Unicast(HTTP)

o Desis =2 UDP/SPTS

FTA/Scrambled
Satellite Source

VOD Source

DVB-T/T2 DVB-T/T2 Receiver | JDP/SPTS
FTA/Scrambled 4
Wireless Source A \ / 1
Multiple Interface SD/HD Encoder !
ﬁ_‘ RlEl pesslp- Core Switch(Gigabit) IPTV Server Hotel PMS
HOSO With Dexin | T
Local Source IPTV software %
SD/HD Encoder UDP/SPTS
Internet Source s
)
Gigabit Switch Gigabit Switch " Gigabit
w .
: Users (1~N) : : Users (1~N) : : Users (1=N) |
! smart v STB with APK ! : Smart TV STB vith APK : Smant TV STB with APK:
1 ! 1 1
1 ! 1 1
1 ! 1 1
1 ! 1 1
1 ! I |





image5.jpeg
Live/VOD Programs Multicast(UDP)

(Z .E.} DVB-S/S2

FTA/Scrambled
Satellite Source

e DVB-T/T2
Wireless Source
Multiple Interface SD/HD Encoder UDP/SP
T i =

UDP/SPTS

DVB-T/T2 Receiver __ UDP/SPTS

o

"

Core Switch(Gigabit) IPTV Server Hotel PMS
— With Dexin T
Local Source g IPTV software =
@_ SD/HD Encoder UDP/SPTS e
)
Gigatsit Switch (IGMP protocol) Gigabit Switch (IGMP protocol) Gigabit Switch (IGMP protocol)
w -
_______________ 1 R R | T e
: Users (1~N) H Users (1-N) \ : Users (1~N) H
pr— STB with APK : SHEHTV STB with APK : : SHEHT STB with APK :
: ! e P ! ! |
| ! ! |
| ! ! 1
| ! ! |
1 ! ! |





image6.jpeg
Hotel

Function List:
Live

VOD

Hotel Intro
Dining
Sceneries
Housekeeping
APPS
Checking out

Live

VOD,

Timeshift
Medical Guide
Clinical Course
Doctor Intro
Phone

APPS

Live
VOD
Timeshift
Phone
APPS





image7.jpeg
Booting Ad Home-Text Ad

welcomewelcomewelc¢orméwelcon

m_ e

|

LOGO

IHRIR —
Current &N = i
NextBHB : RIGRE





image2.jpeg




image3.jpeg




image1.png
FMuser




