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2020 April News: SMS APP based on Smart Phone is issued.
FMUSER Ensurity CAS provides secure content protection for digital TV systems. It features SMS APP subscriber management via smartphones and supports DVB standards. The system enables remote authorization and scalable business operations. Ideal for broadcast operators and interactive TV service providers requiring robust content security. 
Key feature
Delivers remote authorization for operational flexibility
Solution Guide
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Why choose Ensurity
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Total Solution
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Specification
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Main Functions Overview
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SMS Integrated
 
ITP Software India PVT Ltd
Reliablesoft Technologies Pvt. Ltd
Aplomb Tecnology
Paycab Solution Pvt. Ltd
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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Rely on SMS APP in Smartphone,
operators can stay at home to order
products/recharging etc for the
subscribers by smartphone.(Optional)
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Hardware Requirement

—

Hard disk: the free space is 2GB and above

Hard disk number: 2 (Raid1)
Network card: 1GB Network Card x2

Encryption Module encryption dog *1

Encryption hardware: encryption dog *1(in
the case of SMS APP,
optional)

SMS APP in Smartphone

I1SO 11.0 or above (Searching Ensurity to
download the APP from Apple Store)

Android 5.0 or above (APK)

Software Requirement
—

Function Software:

CAS Software

Operator ID based CAS Software (Ensurity 2.0)
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