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Product overview
The FUQ-72XX series delivers FPGA-processed FM stereo signals with LDMOS amplification, featuring adjustable 10W–10kW RF output and AGC stability (±0.1dB). Its dual-transmitter redundancy with coaxial switching ensures 24/7 operation, compliant with GB/T4311-2000/GY/T169-2001 standards. The 4U rack-mount design supports NMS control for broadcast centers and emergency alert systems. 
Key feature
Integrated lightning protection (10kV surge resistance) 
Technical Specifications
	S/No.
	Item
	Unit
	Technical Index
	Remark

	1
	Output Power
	W
	500
	 

	2
	Frequency
	MHz
	1kW≤
	65.5~87; 87~108
	 

	
	
	
	1kW＞
	87～108
	

	3
	Frequency deviation
	Hz
	≤500
	 

	4
	Sparious Radiation
	dB
	≤-70
	 

	5
	parasitic amplitude modulation noise
	dB
	-60
	 

	6
	Pilot frequency deviation
	Hz
	±1
	 

	7
	S signal 38kHz Residual component
	dB
	＜-40
	 

	8
	Deviation (100% modulation)
	kHz
	±75
	 

	9
	pre-emphasis
	µs
	50
	 

	10
	Distortion (100% modulation)
	L
	％
	＜0.2
	 

	
	
	R
	
	
	

	11
	Frequency response (without emphasis, de-emphasis)
	L
	dB
	±0.2
	 

	
	
	R
	
	
	

	12
	Frequency response (with emphasis, de-emphasis)
	L
	dB
	±0.2
	 

	
	
	R
	
	
	

	13
	SNR (100% modulation)
	L
	dB
	≥75
	 

	
	
	R
	
	
	

	14
	L/R Separation
	L   R
	dB
	＞70
	 

	
	
	R   L
	
	
	

	15
	L/R level diffrence
	dB
	＜0.1
	 


 
Specifications and Environment Conditions
	Item
	Item
	Technical Requirements
	Remark

	Output and Input Specifications
	RDS input
	BNC interface(57KHz)
	 

	
	Input interface
	XLR, AES/EBU(Optional)
	 

	
	Output interface
	L29-50K
	 

	Environment condition
	Working temperature
	-20～+50℃
	 

	
	Storage temperature
	-30～+75℃
	 

	
	Relatively humidity
	＜95% (25℃ no condensation)
	 

	
	Cooling mode
	inside forced air cooling
	 

	
	atm press
	86～106kPa
	 

	
	power supply
	AC, 100～264V/50Hz
	 

	
	machine room
	Less dust, shock-free
	 

	
	Demission
(L×W×H)
	10~30W
	482×420×44mm
	 

	
	
	100W
	482×420×88mm
	

	
	
	300~1kW
	482×560×176mm
	

	
	
	3kW
	600×800×1080mm
	

	
	
	5kW
	600×1050×1695mm
	

	
	
	10kW
	650×1050×1695mm
	


 
System Principle
 [image: IMG_256]
 
Order Information
	DFT-7211: 10W
	DFT-7212: 100W
	DFT-7213: 1kW
	 
DFT-7214: 10kW

	DFT-7231: 30W
	DFT-7232: 300W
	DFT-7233: 3kW
	

	DFT-7251: 50W
	DFT-7252: 500W
	DFT-7253: 5kW
	


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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