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FMUSER FUQ-NEP10 IP Gateway 8-12 HD-SD Program Conversion SRT-HTTP-UDP-RTP-RTSP-HLS to RTMP Dual Ethernet IP Anti-Jitter Broadcast IPTV Headend [image: 3EEECN_20230727102009][image: IMG_256]
Product overview
The FMUSER FUQ-NEP10 IP Gateway converts broadcast IP streams between SRT/HTTP/UDP/RTP/RTSP/HLS protocols with RTMP output. It processes 8-12 concurrent HD/SD programs at 8Mbps using IP anti-jitter technology. Dual Ethernet ports (1x full I/O, 1x low-bitrate input) enable flexible deployment. Managed via web-based NMS, this 1RU device suits multi-screen IPTV headends and hybrid broadcast-OTT systems. 
Key feature
IP anti-jitter: Ensures stable stream transmission 
IP Protocol Conversion
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General Principle Chart
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Specifications
	IP Input
	IP input through Ethernet1/ Ethernet2 over SRT, HTTP, UDP, RTP/RTSP and HLS.

	IP output
	IP output through Ethernet1 over SRT, HTTP, UDP, HLS, RTMP and RTP/RTSP.

	System
	Support about 8-12 HD/SD programs (Bitrate:8Mbps) conversion

	
	Web-based NMS management through Ethernet port

	General
	Demission
	180mm×110mm×40mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz



Test data for reference:
	[bookmark: OLE_LINK31]Protocol conversion
	Bit-Rate
	Programs

	UDP to SRT/HTTP/RTP/RTSP/HLS/RTMP
	3Mbps
	20

	UDP to SRT
	8Mbps
	10

	UDP to HTTP
	
	12

	UDP to RTP/RTSP
	
	12

	UDP to RTMP
	
	12

	UDP to HLS
	
	12



	Protocol conversion
	Bit-Rate
	Programs

	SRT to UDP/RTP/RTSP/HLS
	3Mbps
	20

	SRT to UDP
	8Mbps
	12

	SRT to RTP/RTSP
	
	12

	SRT to HLS
	
	12


 
 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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