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Product Overview
The FMUSER IPTV System is a multifunctional platform supporting Live TV, VOD (1080P/60Hz), CAS, and 	PMS integration via IP output. It processes satellite/cable signals and hotel-generated content through 	hardware decoding and ad insertion. The 1U rack-mountable unit is controllable via web-based NMS, 	designed for hotels and hospitals to enhance guest services and operational workflows.
Key feature
Features web-based NMS control for centralized system administration
Functions
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Advantages
Live Channel/Playback
· Support HD/SD cable channel, satellite channel and hotel self-made channel broadcast
· Support playback shifted live channel, shifting duration can be customized
 
VOD
· Support up to 1080P/60Hz full HD video
· Support hardware decoding, play HD videos smoothly
· Classify movie files, convenient for selecting
 
Advertisement System—Value added Services
· Hotel or hospital owners can set up advertisement business to increase revenues. 
· Ad modes include booting ad, VOD ad, pictures and text ad etc
 
Mass HD Programs
· Support 1080P/60Hz full HD video
· Mass resource of Video on Demand including movies, entertainments, factual shows and etc
 
CAS (Conditional Access System)
· Our conditional access system gives the customer choice over pay channels and which prevent unauthorized access.
 
PMS integration
· Support IPTV system integrate with hotel PMS
 
IPTV Server Recommended configuration
	Number of STB
	Server Configuration
	Switch
	Remarks

	300≤
	IPTV Server：Dell730
	CPU: Xeon E5-2609 v3
Memory:16G
Network: Four-port Gigabit NIC
Storage：configure as needed (suggest 1T above)
	1 set
	Gigabit
	If the UDP protocol is adopted in live services, switches of access layer should support IGMP protocol.

	500≤
	IPTV Server：Dell730
	CPU: Xeon E5-2640 v4
Memory:32G
Network: Four port Gigabit NIC
Storage：configure as needed (suggest 1T above)
	1 set
	Gigabit
	 (1) If the system has high requirements for VOD services and video playback services, like online VOD is with over 300 terminals, it is strongly suggested to configure a storage server.
(2) If the UDP protocol is adopted in Live services, Switches of Access Layer should support IGMP protocol.

	
	IPTV Storage Server：OceanStor S2200T
	Cache：16G
Storage：configure as needed
	1 set (Optional)
	
	

	＞500
	IPTV Server：Dell730
	CPU: Xeon E5-2640 v4
Memory:32G
Network: Four port Gigabit NIC
Storage：configure as r needed (suggest 1T above)
	1 set
	Gigabit Switches and Switches of Access Layer should support  IGMP protocol
	If the system has high requirements for VOD services and video playback services, like online VOD is with over 300 terminals, it is strongly suggested to configure a storage server. The specific model should consult storage server supplier.

	
	IPTV Storage Server
	 
Storage：configure as needed
	1 set (Optional)
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                            Main Interface                                                         VOD
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                           Hotel Introduction                                                       Food Ordering
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                         Scenery Introduction                                                    Service
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                                APPS                                                                     Setting
         
                                                   


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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