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The FMUSER FUQ-200C integrates multiplexer, scrambler, and modulator functions, delivering up to 128 DVB-C QAM channels via RF ports. It processes input signals through SFP+ ports, supporting TS over UDP/RTP and multicast protocols. Housed in a 1U chassis, it features web-based management for easy control. Ideal for broadcast systems requiring high-density signal processing.The device is equipped with 1 (or 2) 64ch QAM card and characterized with dual RF output ports on each card to broaden the bandwidth for QAM carriers. Its high density helps operators to save cost to the most extent.
 
Key feature 
High-Density Design: Features a 1U chassis with plug-in cards for up to 128 non-adjacent carrier outputs.  
Advanced Processing: Supports multiplexing, scrambling with 6 CAS Simul-cryption, PCR adjusting, PID remapping, and PSI/SI editing.  
Flexible Interfaces: Includes 3 SFP+ (10G)/SFP (1G) ports for TS over UDP/RTP and multicast.  
Web-Based Management: Enables easy monitoring and configuration via a network interface.  
 
Inner Principle Chart (two cards)
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Carrier Setting Illustration (per card)
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Specifications
	Input
	Input
	Max 512 IP in per card through SFP+/SFP ports 1-3

	
	Transmission Rate
	Max 9600Mbps for each 10G SFP+/SFP input

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	Mux
	Max PIDs Remapping
	256 per output channel

	
	Functions
	PID remapping (auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Scrambling
	Max simulcrypt CA
	6

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	Modulation Standard
	EN300 429/ITU-T J.83A/B/C

	
	Constellation
	J.83A
	Constellation :16/32/64/128/256QAM

	
	
	
	Bandwidth :8M

	
	
	J.83B/C
	Constellation :64/256QAM

	
	
	
	Bandwidth :6M

	
	QAM Channel
	64/128 non-adjacent carrier outputs, 384Mbps bandwidth for each RF port

	
	Symbol Rate
	3600~7000Ksps, 1ksps stepping
5057Ksps (J.83B, 64QAM) ; 5361Ksps (J.83B, 256QAM)

	
	Constellation
	16, 32, 64 , 128, 256QAM

	
	FEC
	RS (204, 188)

	RF Output
	Interface (per card)
	2 F type output ports for 64 carriers, 75Ω
Carrier 1~32 out thru RF1, 33~64 thru RF2

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	MER
	≥ 40dB

	TS output
	Per Daughter QAM Card
	64 IP output over UDP/RTP/RTSP, unicast/multicast,
through SFP+/SFP ports 1-3

	System
	Web-based Network management

	General
	Dimension
	420mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz; or AC 220V±10%, 50/60Hz
Redundancy power supply (optional as per order)

	
	Consumption
	50W(1 daughter QAM card)/75W(2 daughter QAM cards)


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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