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The FMUSER FUQ-200E is a 10G IP QAM processor integrating multiplexer, scrambler, and modulator functions. It processes signals through multiplexing, scrambling, and modulation, supporting up to 112 DVB-C QAM channels with 3 SFP+(10G)/SFP(1G) ports and 2 GE ports. Housed in a 1U chassis with modular card slots, it features web-based network management and is ideal for cable television headends and broadcast systems requiring high-density processing.This processor is equipped with 2 card slots to load 32ch or 48ch or 64ch QAM card. Its high density helps operators to save cost to the most extent.
 
Key feature
Enables web-based network management for remote monitoring and control.
 
Inner Principle Chart (Example: one 64qam card + one 48qam card)
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Carrier Setting Illustration (Example: 64qam card)
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Specifications
	Input
	Input from Front Panel
	Max 512 IP in per card through SFP+/SFP ports 1-3 and 2 GE ports

	
	Input from Daughter Card
	2*512 IP in from 2 GE ports (SFP port optional)--32/48 QAM

	
	Transmission Rate
	Max 9600Mbps for each 10G SFP+/SFP input

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	Mux
	Max PIDs Remapping
	256 per output channel

	
	Functions
	PID remapping (auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Scrambling
	Max simulcrypt CA
	6

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	Modulation Standard
	EN300 429/ITU-T J.83A/B/C

	
	Constellation
	J.83A
	Constellation :16/32/64/128/256QAM

	
	
	
	Bandwidth :8M

	
	
	J.83B/C
	Constellation :64/256QAM

	
	
	
	Bandwidth :6M

	
	QAM Channel
	32/48/64/96/112 non-adjacent carriers output,
384Mbps bandwidth for each RF port

	
	Symbol Rate
	3600~7000Ksps, 1ksps stepping
5057Ksps (J.83B, 64QAM) ; 5361Ksps (J.83B, 256QAM)

	
	Constellation
	16, 32, 64, 128, 256QAM

	
	FEC
	RS (204, 188)

	RF Output
	Interface (per card)
	1 or 2 F type output ports for 32/48/64 carriers card, 75Ω.
32ch qam card : all Carrier out thru one RF port
32ch/48ch qam card : Carrier 1~16/1~24 out thru RF1, 17~32/25~48 thru RF2
64ch qam card : Carrier 1~32 out thru RF1, 33~64 thru RF2

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	MER
	≥ 40dB

	TS output
	Per Daughter QAM Card
	32/48/64 IP output over UDP/RTP/RTSP, unicast/multicast,
through SFP+/SFP ports 1-3 or GE ports RJ45

	System
	Web-based Network management

	General
	Dimension
	420mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz ; or  AC 220V±10%, 50/60Hz

	
	Consumption
	50W(1 daughter QAM card)/75W(2 daughter QAM cards)


 
 
Order Guide
	Options Available
	Combinations

	32ch QAM out
	32qam card * 1

	48ch QAM out
	48qam card * 1

	64ch QAM out
	64qam card * 1

	96ch QAM out
	64qam card * 1 + 32qam card *1

	112ch QAM out
	64qam card * 1 + 48qam card *1


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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