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The FUQ-200F integrates multiplexer, scrambler, and modulator in a 1U chassis, with IP inputs via SFP+, SFP, and GE ports to output up to 192 DVB-C QAM carriers. It processes IP streams using CAS encryption and PSI/SI editing for signal modulation. This modular solution features QAM cards (32/48/64ch) and web-based control for easy operation. Ideal for broadcast headend and cable TV systems requiring high-density signal processing.This processor is equipped with 3 card slots to load 32ch or 48ch or 64ch QAM card. Its high density helps operators to save cost to the most extent.
 
Key feature 
Supports modular QAM cards (32/48/64ch) in 1U for high-density output.  
Features IP inputs via 4× SFP+ (10G), 4× SFP (1G), and 12× GE ports.  
Enables multiplexer/scrambler functions with up to 6 CAS encryption standards.  
Generates 192 non-adjacent DVB-C QAM carriers via J.83A/B/C modulation.  
Provides web-based control for RF output (-20dBm~+10dBm) and symbol rates (3600-7200Ksps).  
 
Inner Principle Chart (Example: one 64qam card + one 48qam card + one 32qam card)
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Carrier Setting Illustration (Example: 64qam card)
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Specifications
	Input
	IP Input
	Max1024 IP inputs per card through 4 SFP+, 4 SFP and 12 GE ports in the front panel and 2 SFP ports in the card itself

	
	Transmission Rate
	Max 9600Mbps for each 10G SFP+ input/Max 960Mbps for each GE and SFP input

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	Mux
	Max PIDs Remapping
	256 per output channel

	
	Functions
	PID remapping (auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Scrambling
	Max simulcrypt CA
	6

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	Modulation Standard
	EN300 429/ITU-T J.83A/B/C

	
	Constellation
	J.83A
	Constellation :16/32/64/128/256QAM

	
	
	
	Bandwidth :8M

	
	
	J.83B/C
	Constellation :64/256QAM

	
	
	
	Bandwidth :6M

	
	QAM Channel
	32/48/64/80/96/112/128/144/160/176/192 non-adjacent carriers output,
384Mbps bandwidth for each RF port

	
	Symbol Rate
	3600~7200Ksps, 1ksps stepping
5057Ksps (J.83B, 64QAM) ; 5361Ksps (J.83B, 256QAM)

	
	Constellation
	16, 32, 64, 128, 256QAM

	
	FEC
	RS (204, 188)

	RF Output
	Interface (per card)
	2 F type output ports for 32/48/64 carriers card, 75Ω.
32ch/48ch/64ch qam card : Carrier 1~16/1~24/1~32 out thru RF1, 17~32/25~48/33~64 thru RF2

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	MER
	≥ 40dB

	TS output
	Per Daughter QAM Card
	32/48/64 IP output over UDP/RTP/RTSP, unicast/multicast,
through 4 SFP+ ports, 4 SFP ports and 12 GE ports in the front panel

	System
	Web-based Network management

	General
	Dimension
	480mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz ; or  AC 220V±10%, 50/60Hz

	
	Consumption
	About 200W (3 daughter QAM cards)


 
Major Technical Comparison
	 
	DHP200D
	DHP200E

	Card Number
	Max 2
	Max 3

	SFP+/SFP/RJ45 ports in the front panel
	3 SFP+(10G)/SFP(1G) ports and 2 GE ports
	4 SFP+ (10G)/4 SFP(1G) ports and 12 GE ports

	Max Carriers number
	112
	192

	Inner connector GE ports
	6
	12

	DATA Port in card
	DepeFU on card spec
	2 SFP ports as input per card


 
Order Guide  
· Card Type Option: 32, 48 or 64 QAM card
· Card Number Option: 1, 2 or 3 pcs
· SFP ports option in card: With or Without
· PSU option: 1*220VAC or 2*220VAC not hot-swapping PSU
 
 
 

 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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