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The FMUSER FUQ-2500E Agile Modulator offers RF modulation with 1 audio (L/R) and 1 video (CVBS) input, plus configurable RF output. It processes signals using video input AGC for stability. This unit features a 19-inch 1U rack-mount design and keyboard/LCD operation with online upgrade. Ideal for hotels, communities, and entertainment venues.
Key feature
- Supports 1 audio (L/R) and 1 video (CVBS) input for versatile connectivity.  
- Configurable RF output (47-870MHz) with test port and ±5kHz accuracy.  
- Features video input AGC and compatibility with PAL B/G, PAL D/K, NTSC, SECAM standards.  
- Enables keyboard and LCD operation with online upgrade capability.  
- Integrates 19-inch 1U rack-mount design for easy installation.  
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Specifications
	Input
	1* audio (L/R) input and 1*video (CVBS)

	Video
	A/V ration
	-10~-20dB

	
	Input level
	1VPP

	
	Video clamping capacity
	≥26dB

	
	Color / light delay difference
	≤45nS

	
	Differential gain
	≤2% (Modulation 87.5%)

	
	Differential phase
	≤2° (Modulation 87.5%)

	
	SNR
	≥50dB

	
	Image carrier drift
	≤5kHz

	
	2T-K impulse ratio
	≤4%

	
	Flatness in band
	≤1dB

	Audio
	Pre-emphasis of audio
	50μs

	
	Input level
	0.7V

	
	SNR
	≥60dB

	
	Flatness in band
	≤1dB

	
	Distortion degree
	≤0.5%

	
	Audio modulation frequency offset
	± 50kHz

	
	V/A interval
	According to TV System standard

	RF Output
	Interface
	1 F typed output port, 75Ω

	
	Frequency range
	47~870MHz, 1kHz step

	
	TV system standard
	PAL B/G, PAL D/K, NTSC, SECAM

	
	Output return loss
	≥14dB

	
	Output level
	≥113dBμV

	
	Output level adjustable range
	0~16dB

	
	Error of video/audio carrier interval
	≤5 kHz

	
	Carrier to noise ratio (C/N)
	≥62dB

	
	Output suppression
	≥60dB (≥130dBuV testing)

	
	Flatness in band
	≤1dB

	
	Frequency accuracy
	≤5kHz

	
	Adjacent Frequency suppression
	≥45dB

	System function
	Keyboard and LCD operation

	
	Multiple languages

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482*256*44mm

	
	Environment
	-10~45℃(work); -20~80℃ (storage）

	
	Power requirements 
	AC 90-264V, 50Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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