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FMUSER FUQ-3214B Professional Encoder 4 CVBS Inputs MPEG-2 PAL-NTSC SD Video Encoding IP Output UDP-RTP MPTS-SPTS for CATV Satellite Terrestrial TV Headends
[image: 3EEECN_20170619110009]
· [bookmark: _GoBack][image: IMG_261]
Product Overview
The FMUSER FUQ-3214B is a multi-channel SD encoder and multiplexer with 4 CVBS inputs and IP output via UDP/RTP. It encodes video in MPEG-2 format and audio in MPEG-1 Layer 2 or DD AC3 (2.0), then multiplexes signals into MPTS or SPTS streams. Controlled via a web-based interface for real-time monitoring. Ideal for CATV, satellite, and terrestrial digital TV systems. 
Key feature
- Supports 4 CVBS inputs with MPEG-2 video encoding for PAL/NTSC SD formats.  
- Provides dual audio encoding: MPEG-1 Layer 2 and DD AC3 (2.0) at 48kHz sampling.  
- Delivers multiplexed IP output via UDP/RTP for MPTS and SPTS streams.  
- Includes broadcast enhancements like Null PKT Filter, CC, and logo insertion.  
- Features web-based control for real-time monitoring and updates.  
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Technical Specification
	Input
	4 CVBS inputs , RCA interface

	Video
	Resolution
	Input
	Output

	
	
	720*576
	720×576_50i, 704×576_50i,
640×576_50i, 352×288_50i,
320×288_50i, 176×288_50i,176×144_50i

	
	
	720*480
	720×480_60i, 544×480_60i, 352×480_60i, 352×240_60i, 320×240_60i, 176×240_60i, 176×120_60i,

	
	Encoding
	MPEG-2

	
	Bit-rate
	0.5Mbps~8Mbps per channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	GOP_0_B, 1B, 2B,3B

	
	Aspect Ratio
	4:3; 16:9

	Audio
	Encoding
	MPEG-1 Layer 2, DD AC3 (2.0)

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	-12~+40 adjustable

	
	Bit-rate
	64Kbps, 128Kbps,192kbps,256kbps,320kbps,384kbps each channel

	Stream output
	IP (1*MPTS and 4*SPTS) output over UDP and RTP, 1000 Base-T Ethernet interface (multicast)

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Approx weight 
	5kg

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
  


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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