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Product Overview
The FMUSER FUQ-3214C is a multi-channel SD encoder supporting 4/8/12 CVBS or SDI inputs with MPEG-2 and H.264 encoding. It processes signals by encoding and multiplexing to TS for IP output. This modular device fits in a 1U chassis with up to three independent modules, controlled via a web-based interface. Ideal for CATV digital headends and broadcast distribution systems. 
Key feature
The FMUSER FUQ-3214C is a multi-channel SD encoder supporting 4/8/12 CVBS or SDI inputs with MPEG-2 and H.264 encoding. It processes signals by encoding and multiplexing to TS for IP output. This modular device fits in a 1U chassis with up to three independent modules, controlled via a web-based interface. Ideal for CATV digital headends and broadcast distribution systems. 
Principle Chart (per daughter module)
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Technical Specification
	Input
	4/8/12 CVBS input , DB15-To-RCA interface ---OptionⅠ
4/8/12 SDI input, BNC interface ---OptionⅡ

	Video
	Resolution
	Input
	Output

	
	
	720*576 @50i
	720*576/352*288/320*240/320*180/176*144
/160*120/160*90@50Hz

	
	
	720*480 @60i
	720*480/352*288/320*240/320*180/176*144
/160*120/160*90@60Hz

	
	Encoding format
	MPEG-2, MPEG4 AVC/H.264

	
	Bit-rate
	0.5~5Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IPPP, IBPBP, IBBPB, IBBBP

	
	Aspect Ratio
	4:3, 16:9

	Audio
	Encoding format
	MPEG1 Layer 2, LC-AAC, HE-AAC

	
	Sampling rate
	48KHz

	
	Bits per sample
	32-bit

	
	Audio Gain
	-20~+12 adjustable

	
	Bit-rate
	48Kbps~384Kbps (each channel)

	Stream output
	IP (1*MPTS and 4*SPTS) output over UDP and RTP/RTSP (unicast/multicast) per module,100M/1000M self-adaption

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
Technical Comparison
	 
	FU-4339A
	DX3214B-4/8/12

	Chipset
	Magnum
	Magnum

	Input interface
	8× CVBS, BNC
	4/8/12× CVBS Optional, RCA interface
4/8/12×SD-SDI , BNC interface
(Modular design with each module supporting 4 channels, one chassis supporting up to 3 modules)

	
	8×SD-SDI input with embedded audio
	

	Bitrate
	0.25~15Mbps for H.264 encoding
0.5~15Mbps for MPEG-2 encoding
	0.5~5Mbps for both H.264 and MPEG-2 encoding

	ASI In&Mux
	1 ASI IN
	N/A

	ASI Output
	2*ASI mirrored Output
	N/A

	IP Output
	· 8 SPTS or 1 MPTS output over UDP (unicast / multicast)
· 10/100Base-T Ethernet interface * 1
· one data port for all channels
	· 4 SPTS and 1 MPTS output over UDP and RTP/RTSP for each module (unicast/multicast)
· 1000 Base-T Ethernet interface*1/2/3
· one data port for one module (4 channels)

	OSD insertion
	N/A
	Support logo/caption/QR Code insertion

	Operation
	· Web-based NMS
· SNMP (Optional)
· Front panel with LCD+Key board
	· Web-based NMS

	Control Mode
	One NMS port for all channels
	One NMS port for each module (4 channels)


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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OSD (Logo/PPT/Caption/QR Code) Insertion
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Dexin OSD Insertion Standard

’ Customization: Showing time &Displaying effect

’ Easy operation: fresh man learn it in few minutes

LOGO Insertion

Support jpg/jpeg/bmp/gif/png file

Support multi pictures compressed into a zip file and display pictures in a dynamic way

Multi transition type: Continuous/ Fade Inout/ Blind window/ Square
Custom live/wait time of pictures

Custom transparency D& /NG
Custom size DE OING—> vesin

Drag to move to any position

Transparent background
(hollow out) with png/gif
type picture

White background with
ipg/ipeg/bmp type picture

Caption Insertion — QR Code Insertion

Custom running direction & 9 Input URL and create immediately

EmgE
Custom running speed .Q_ D Support add text at top or bottom &
Custom font color/size/weight . A A ‘D Custom size: 40*40 -- 400*400
o]
Support multi languages - = €- 9 Support add logo at the center

Custom showing period and text length € @ Drag to move to any position

Custom background, transparency or any color €

Drag to move to any position




image7.jpeg
CVBS/SDI #1

_* MPEG-2/MPEG4 Encoding

MPEG-2/MPEG4 Encoding

CVBS/SDI #4

MPEG-2/MPEG4 Encoding
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Dexin Digital, the authorized licensee, takes you into a new digital life.
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