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The FUQ-3504 IP Multiplexer integrates 4 ASI and 768 IP inputs, multiplexing them into 4 MPTS outputs. It processes signals with PSI/SI auto-generation, PID remapping, and PCR adjustment. Managed via web-based NMS through a 10/100M Ethernet port. Ideal for CATV broadcasting and digital TV head-end systems. 
Key feature
Supports 4 bi-directional ASI ports with manual direction control.  
Features 768 UDP/RTP inputs via GE1, GE2, and DATA ports.  
Delivers 4 MPTS outputs through GE1, GE2, and DATA ports.  
Enables PCR adjustment, PID filtering/remapping, and PSI/SI editing.  
Provides web-based NMS management via 10/100M Ethernet port.
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Specifications
	Input / Output
	4 bi-direction ASI ports: max 4 ASI input/output, BNC 75Ω
3 bi-direction Data ports (RJ45)
768 IP inputs over UDP/RTP (256 IP inputs thru GE1, GE2 and DATA port respectively)
4 MPTS outputs over UDP/RTP thru GE1, GE2 and DATA port
100/1000Mbps self-adaption for all data ports

	
	Packet format
	204/188 self-adaption for input, 204/188 is settable for output

	
	Output TS Mode
	bytes/packets

	Re-multiplex
	Max PID numbers
	748 PID numbers for GE1

	
	
	748 PID numbers for GE 2

	
	
	748 PID numbers for DATA port and 4 ASI ports together

	
	Functions
	PID re-mapping

	
	
	PCR accurate adjusting

	
	
	Automatic generating PSI/SI table

	
	PID transparent
	PID transparent and mapping achievable

	System
	Web management:10/100M NMS port

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×300mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤40W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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