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The FMUSER FUQ-3512A DVB-T Modulator provides DVB-T (EN300744) compliant modulation with RF output. It processes signals for digital transmission and features web-based management for control. Ideal for MFN and SFN digital TV networks. 
Key feature
Supports DVB-T (EN300744) compliance for reliable broadcasting.  
Features SFN and MFN network operation flexibility.  
Delivers MER ≥42dB with superior phase noise performance.  
Provides RF output at 50-1000MHz with 1Hz tuning precision.  
Includes adaptive non-linear digital pre-distortion (DPD) for efficiency optimization.   
Specifications
	Input
	2channels ASI input& 2 IP input, can only select 1 input as source, but all 4 inputs ports are hot backup
IP with UDP/RTP protocol, with Multicast/Unicast
IP with PCR adjust feature also

	
	GPS 10Mhz reference clock input, BNC port

	
	GPS 1PPS input, BNC port

	
	1 RF input for DPD  -25dbm~+5dbm

	Modulation
	Standard
	EN300 744

	
	FFT
	2K, 8K

	
	Bandwidth
	5M, 6M, 7M, 8M

	
	Constellation
	QPSK, 16QAM, 64QAM

	
	Guard interval
	1/4, 1/8, 1/16, 1/32

	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	RF output
	Interface
	N type, 50Ω impedance

	
	 
	 

	
	RF range
	50~1000MHz，1hz step

	
	RF output level
	-15dbm~+5dbm, 0.1db step

	
	RF level offset
	-3dbm~+3dbm, 0.1db step

	
	MER
	≥ 42db

	ASI output
	2 ASI ports output for the passthrough of the input ASI Signal, both ASI out are the same

	Non-linear DPD
	over 10db ACPR improvement (normally)

	System
	LCD display & keyboard operation, web management

	
	Software upgrading through NMS port

	General
	Demission (W*L*H)
	440mm×414mm×44.5mm

	
	Weight
	4.9kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 110V±10%, 50/60Hz or AC 220V±10%, 50/60Hz

	
	Power Consumption
	To be tested


 
 Principle Chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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