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 The FUQ-3514 Multiplexer Scrambler provides multiplexing and scrambling functions with 4 ASI inputs, 128 IP inputs, and 4 MPTS outputs. It processes signals through PSI/SI auto-generation, PID re-mapping, service filtering, and PCR adjusting. Managed via web-based NMS, this device is ideal for CATV broadcasting systems, ensuring efficient integration and reliable performance.  
Key feature
Supports up to 4 ASI inputs/outputs and 128 IP inputs with 4 MPTS outputs.
Enables scrambling compliant with ETR289, ETSI 101 197, and ETSI 103 197, supporting up to 4 simulcrypt CAs.
Allows PID management including filtering, re-mapping up to 512 PIDs per channel, and PSI/SI rebuilding.
Features PCR adjusting, buffer memory for overflow protection, alarming function, and web-based NMS management.
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Specifications
	Input / Output
	4 bi-direction ASI ports: max 4 ASI input/output, BNC 75Ω
3 bi-direction Data ports (RJ45): 128 IP input over UDP/RTP
4 IP (MPTS) output over UDP/RTP/RTSP
100/1000Mbps self-adaption

	
	Input Packet format: 204/188 self-adaption

	
	ASI: Max output bit-rate: 200Mbps (Each channel)

	Mux
	Max PIDs
	512 per channel

	
	Functions
	PID re-mapping

	
	
	PCR accurate adjusting

	
	
	Automatic generating PSI/SI table

	
	PID transparent
	Any PID transparent and mapping achievable

	Scrambling
Parameters
	Max simulcrypt CA
	4

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Scramble Channel
	1

	
	Connection
	Local/remote connection

	System
	Web-based management

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×300mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤40W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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