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Product Overview
The FUQ-3515 ASI TS Switcher provides 1 main + 2 backup ASI inputs and 2 independent ASI outputs for transport stream redundancy. It performs automatic failback switching based on TS packet integrity monitoring (bitrate/sync/continuity). This 1RU rack-mount unit supports web-based control and firmware upgrades. Ideal for broadcast headend redundancy and cable TV signal backup systems. 
Key feature
WEB-based management: Remote control via HTTP/HTTPS with upgrade support 
Specifications
	Input
	3 ASI input: ASI 3 is main stream, ASI 2 is secondary stream (backup 1), ASI 1 is third stream (back up 2)

	Output
	2 ASI output: ASI 4 output bypass, ASI 5 loop out ASI 3

	Interface
	BNC interface

	TS Package Format
	188

	ASI in/out bitrate
	1~210Mbps

	System
	language
	English/Chinese

	
	Remote Control
	web-server management (WEB)

	
	Upgrade
	Web upgrade

	General
	Size
	482mmx410mmx44mm

	
	Temprature
	0~45℃ (working); -20~80 (Storage)

	
	Power Supply
	110VAC±10%, 50/60Hz
220VAC±10%, 50/60Hz

	
	Consumption
	15W
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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