[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[bookmark: _GoBack]FMUSER FUQ-3516R ISDB-T Modulator Dual ASI-Dual IP Inputs ARIB STD-B31 6MHz Bandwidth Network Control SFN-MFN Broadcasting STB Testing [image: 3EEECN_20200928060507]Product overview
The FMUSER FUQ-3516R ISDB-T Modulator delivers terrestrial digital television broadcasting, featuring dual ASI and dual IP inputs. It modulates signals compliant with ARIB STD-B31 standards, supporting single frequency network (SFN) and multi-frequency network (MFN). With network-based control via WEB interface, LCD, and keyboard, it enables easy management. Ideal for broadcasting network setup and set-top box testing in South American markets like Brazil and Argentina.
Key feature
Enables network control via WEB, LCD, and keyboard for easy upgrades.
 
Specifications
	Input
	2 ASI ports input, one for hot backup, BNC interface

	
	Dual IP input ports over UDP/RTP, Unicast/Multicast, GE ports

	
	1 channel 10MHz reference clock input

	
	1 RF input for DPD  -15.2dbm~+5dbm

	Modulation
	Standard
	ARIB STD-B31

	
	Mode
	mode 1(2k), mode 2(4k), mode 3(8k)

	
	Constellation
	DQPSK, QPSK, 16QAM, 64QAM

	
	External coding
	RS (204，188)

	
	Internal coding
	Convolution (1/2, 2/3, 3/4, 5/6, 7/8)

	
	Guard interval
	1/4, 1/8, 1/16, 1/32

	
	Hierarchy mode
	A、A+B、A+B+C

	
	Time domain interlacing
	mode 1: 0, 4, 8, 16    mode 2: 0, 2, 4, 8
mode 3: 0, 1, 2, 4

	
	Bandwidth
	6MHz

	RF Out
	Connector
	N Type, 50ΩImpedance

	
	RF range
	50~999Mhz，1Hz step

	
	Output level ATT
	-20dbm~+5dbm，0.1db step

	
	MER
	≥ 42db

	Non-linear DPD
	over 10db ACPR improvement (normally)

	linear DPD
	over 10db non-flatness adjustment(normally)

	System
	LCD display & keyboard operation, WEB, Chinese & English operation display

	
	Supporting software upgrading through WEB

	General
	Demission (W*L*H)
	440mm×414mm×44.5mm

	
	Weight
	4.9kg

	
	Temperature
	0~45℃(operation),-20~80℃(storage)

	
	Power supply
	AC 100V~240V,50/60Hz

	
	Consumption
	25W


 
Principle chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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