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Product Overview
The FMUSER FUQ-3532AB integrates encoding, multiplexing, and modulating functions, supporting 32 CVBS inputs, 1 DVB-C tuner, 1 ASI, and 256 IP inputs, with 8 MPTS outputs via IP and 8 RF outputs. It processes signals by encoding with MPEG4 AVC/H.264, multiplexing, and modulating for transmission. Housed in a standard 1U case, it offers web-based management for real-time monitoring and updates. Ideal for DTV broadcasting systems, enabling cost-effective multi-channel distribution in cable and IPTV networks.DX3532SA also supports 1 DVB-C tuner input, 1 ASI and 256 IP input and 8 non-adjacent carriers output through RF output interface and data port output. The device is also characterized with high integrated level, high performance and low cost. This is very adaptable to newly generation DTV broadcasting system.
 
Key feature
Integrated Encoding and Modulating: Combines encoding and modulating in a compact 1U case for efficient processing.  
Versatile Input Support: Accepts 32 CVBS, 1 DVB-C tuner, 1 ASI, and 256 IP inputs over UDP/RTP.  
Advanced Output Capabilities: Generates 8 MPTS outputs via IP and 8 RF outputs for flexible broadcasting.  
Stream Management Tools: Enables PID remapping, PCR adjustment, PSI/SI editing, and logo insertion.  
Web-Based Control: Features real-time monitoring and easy updates via web interface.
 
Principle Chart
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DVB-C RF Out
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DVB-T RF Out
Technical specification
	Input
	32 CVBS inputs , DB15-To-RCA interface

	
	1ASI input port

	
	256 IP (100/1000M)input over UDP and RTP protocol

	
	1 DVB-C Tuner input

	Video
	Resolution
	720×576i (PAL-B, D, G, H, I), 720×480i (NTSC-M, J)

	
	Encoding
	MPEG4 AVC/H.264（HP/MP/BP）

	
	Bit-rate
	1Mbps~5Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IPP(P frame is adjustable)

	Audio
	Encoding
	MPEG-1 Layer 2

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 adjustable

	
	Bit-rate
	64/128/192/224/256/320/384Kbps each channel

	Modulation
	DVB-C
	QAM Channel: 8 non-adjacent carriers output (maximum bandwidth 192MHz)
Standard: EN300 429/ITU-T J.83A/B
MER: ≥40dB
RF frequency: 50~960MHz, 1KHz step
RF output level: -20~+3dBm (87~110 dBµV), 0.1dB step
Symbol Rate: 5.0Msps~7.0Msps, 1ksps step

	
	
	 
	J.83A
	J.83B

	
	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM

	
	
	Bandwidth
	8M
	6M

	
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K, 4K, 8K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥40 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	8*COFDM DVB-T non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20~+3 dBm (87~110 dBµV), 0.1dB step

	Scrambling
Parameters
	Max simulscrypt CA
	4

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Stream output
	IP (8*MPTS) output over UDP and RTP, 100/1000 Base-T Ethernet interface (Multicast/unicast)

	System function
	Network management (WEB)

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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