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The FMUSER FUQ-3902B is a DVB-S2X receiver that integrates demodulation, descrambling, and remuxing, featuring 2 RF tuner inputs and 32 IP inputs supporting UDP/RTP, with IP output. It converts satellite signals into IP streams through efficient processing. This compact unit enables remote control via web-based NMS management. Ideal for broadcast facilities, satellite reception, and IP streaming applications. 
Key feature
- Supports dual DVB-S/S2/S2X tuner inputs for versatile reception.
- Features 32 IP inputs with UDP/RTP support for remuxing.
- Integrates decryption via CAM/CI slots and BISS.
- Enables remote monitoring and control through web-based NMS.
- Allows high PID mapping with up to 256 mappings per input channel.
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Technical specification
	Input
	2*RF (DVBS/S2/S2X), F type
32*IP input for re-mux (UDP/RTP) through data(1000M/100M) ports

	Tuner
	DVB-S
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK 0.5Msps~45Msps

	
	
	Signal Strength
	-65~ -25dBm

	
	
	FEC Demodulation
	1/2, 2/3, 3/4, 5/6, 7/8

	
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK 0.5Msps~45Msps
32APSK0.5Msps~40 Msps

	
	
	FEC Demodulation
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9

	
	DVB-S2X
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps;
8APSK/32APSK: 0.5~40 Msps

	
	
	FEC Demodulation
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10, 23/36, 25/36, 13/18
8APSK: 5/9-L, 26/45-L
16APSK:2/3,3/4,4/5, 5/6, 8/9, 9/10,1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9 

	Multiplexing
	Maximum PID Remapping
	256 PIDs per input channel

	
	Function
	PID remapping (automatically or manually), Accurate PCR adjusting, generate PSI/ SI table automatically

	Descrambling
	CAM/CI Quantity
	2

	
	BISS Mode
	Mode 1, Mode E; up to 120Mbps

	Output
	1*MPTS over UDP and RTP, 1000M/100M Base-T Ethernet interfaces (unicast / multicast)

	System function
	Network management (WEB)

	
	English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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