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FMUSER FUQ-3902B DVB-S-S2-S2X Demodulator Descrambler IP Multiplexer 2 Tuner Inputs 32 IP Stream Outputs UDP-RTP Web-NMS Headend IPTV
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The FMUSER FUQ-3902B is a professional DVB-S/S2/S2X demodulator, descrambler, and IP multiplexer with 2 tuner inputs (950-2150MHz) and 32 IP stream outputs (UDP/RTP). It demodulates satellite signals, decrypts via CAM/CI or BISS, and remuxes up to 32 channels into a single MPTS output. This 1RU rack-mount unit supports DiSEqC control and web-based NMS, ideal for broadcast headends and IPTV distribution. 
Key feature
Web-based NMS for remote configuration and monitoringPrinciple Chart
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Technical specification
	Input
	2*RF (DVBS/S2/S2X), F type
32*IP input for re-mux (UDP/RTP) through data(1000M/100M) ports

	Tuner
	DVB-S
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK 0.5Msps~45Msps

	
	
	Signal Strength
	-65~ -25dBm

	
	
	FEC Demodulation
	1/2, 2/3, 3/4, 5/6, 7/8

	
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK 0.5Msps~45Msps
32APSK0.5Msps~40 Msps

	
	
	FEC Demodulation
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9

	
	DVB-S2X
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps;
8APSK/32APSK: 0.5~40 Msps

	
	
	FEC Demodulation
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10, 23/36, 25/36, 13/18
8APSK: 5/9-L, 26/45-L
16APSK:2/3,3/4,4/5, 5/6, 8/9, 9/10,1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9 

	Multiplexing
	Maximum PID Remapping
	256 PIDs per input channel

	
	Function
	PID remapping (automatically or manually), Accurate PCR adjusting, generate PSI/ SI table automatically

	Descrambling
	CAM/CI Quantity
	2

	
	BISS Mode
	Mode 1, Mode E; up to 120Mbps

	Output
	1*MPTS over UDP and RTP, 1000M/100M Base-T Ethernet interfaces (unicast / multicast)

	System function
	Network management (WEB)

	
	English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
        
   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image2.png




image3.png
Tuner 1

Tuner 2

cAam/cr2 1




image1.png
FMuser




