[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[bookmark: _GoBack]FMUSER FUQ-3904C Receiver Card 4 Tuner Inputs 5 MPTS UDP-RTP Outputs DVB-S-S2-S2X PID Remapping DiSEqC Support Broadcast IPTV Integration
[image: 3EEECN_20200902092009]
Product overview
The FMUSER FUQ-3904C is a professional receiver card supporting DVB-S/S2/S2X standards, featuring four tuner inputs and five MPTS outputs. It processes satellite signals through multiplexing and PID remapping. Managed via web-based NMS for remote control. Ideal for broadcast integration and satellite reception systems.
Key Features
Includes DiSEqC support for enhanced satellite dish functionality. 
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Specifications
	Input / Output
	4 Tuner input, F Type
5 MPTS (4 MPTS out thru bypassing, 1 MPTS multiplexing) out over UDP/RTP thru Data port, 100/1000Mself-adaption, unicast/multicast

	Mux
	Max number of managing PID: 256 (for 1 MPTS out thru multiplexing)

	
	Functions
	PID remapping (automatically/ manually)

	
	
	PID pass-through

	Tuner Section
	DVB-S
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	0.5~45 Msps

	
	
	Constellation
	QPSK

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps
32APSK:0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9,9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	DVB-S2X
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps;
8APSK/32APSK: 0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/8APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10, 23/36, 25/36, 13/18
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10,1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	Signal Strength
	-65 ~ -25dBm

	System
	Web management:100M NMS port

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×328mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤40W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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