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Product overview
The FMUSER FUQ-41013K TransModulator converts satellite signals to terrestrial formats with dual DVB-S/S2/S2X tuners and 2 CAM slots. It processes signals through 2 groups multiplexing and 2 groups DVB-T modulating, including PCR adjusting and PID remapping. Managed via web-based NMS for remote control, it suits broadcasters in TV transmission and terrestrial network deployments.
Key feature
Features dual DVB-S/S2/S2X tuners with 2 CAM slots for secure reception.  
Supports 2 groups multiplexing and 2 groups DVB-T modulating for flexible output.  
Includes accurate PCR adjusting, PID remapping, PSI/SI editing, and A/V PID filtering.  
Enables web-based NMS for remote monitoring and upgrades.  
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Tech Specifications
	Input
	2 DVB-S/S2/S2X Tuners

	Tuner Section
	DVB-S/S2/S2X Tuner 
	DVB-S
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	0.5~45Msps

	
	
	
	Signal Strength
	- 65- -25dBm

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Max input bitrate
	≤129 Mbps

	
	
	DVB-S2
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK: 0.5~45 Msps
32APSK: 0.5~40Msps;

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
 32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤129 Mbps

	
	
	DVB-S2X
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK: 0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~40Msps

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤129 Mbps

	Descrambling
	CAM/CI
	2 sets

	Multiplexing
	Maximum PID Remapping
	256 per input channel

	
	Function
	A/V PID filtering

	
	
	PID Remapping

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/SI table automatically

	Modulation
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	Code Rate
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥42 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	2*DVB-T non-adjacent carriers combined output

	
	
	RF output level
	-28~ -3 dBm (79~104 dbµV), 0.1db step

	System
	Web-based NMS support

	
	Ethernet software upgrading

	General
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 100V±1050/60Hz; AC 220V±10%, 50/60HZ


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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