[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
FMUSER FUQ-41086D HD IRD 8 Tuner Inputs DVB-S-S2-S2X DVB-S2-S2X Outputs UDP-RTP Dual Mode BISS Decryption Diseqc Broadcast IPTV
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Product overview
The FMUSER FUQ-41086D HD IRD supports up to 24 tuner inputs for DVB-S/S2/S2X, DVB-C/T, and ISDB-T standards. It processes signals in Passthrough mode for 8 MPTS output or Mux mode for 2 MPTS / 512 SPTS over UDP/RTP. Managed via web-based NMS, it includes features like Biss decryption and Diseqc function. Ideal for broadcast and IPTV systems.
Key feature
Supports expandable tuner inputs for up to 24 tuners via optional cards, compatible with DVB-S/S2/S2X, DVB-C/T, and ISDB-T.  
Features dual output modes: Passthrough mode for 8 MPTS or Mux mode for 2 MPTS / 512 SPTS over UDP/RTP unicast/multicast.  
Enables advanced PID handling including remapping and pass-through (up to 256 PIDs per channel) exclusively in Mux mode.  
Includes security with Biss decryption (64 keys per tuner) and Diseqc function, managed via NMS.
Inner Principle Chart (Per Card/8 Input): 
Version 1: Passthrough Mode
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Version 2: Mux Mode (MPTS and SPTS output Switchable) 
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Specifications (Per Card/8 Input)
 
	Input / Output
	8 Tuner input (DVB-S/S2/S2X or/and DVB-C/T/T2/ISDB-T), F Type
8 MPTS out thru bypassing over UDP/RTP thru Data port (Version 1)
100/1000Mself-adaption, unicast/multicast

	Mux (Version 2)
	Max number of managing PID: 256 (for 2 MPTS out thru multiplexing) or 512 SPTS out

	
	Functions
	PID remapping (automatically/ manually)

	
	
	PID pass-through

	Tuner Section
	DVB-S
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	0.5~45 Msps

	
	
	Constellation
	QPSK

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps
32APSK:0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9,9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	DVB-S2X
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps;
8APSK/32APSK: 0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/8APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10, 23/36, 25/36, 13/18
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10,1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	
	Signal Strength
	-65 ~ -25dBm

	
	DVB-C
	Input Frequency
	60 ~890 MHz

	
	
	Standard
	J.83A, J.83C
	J.83B

	
	
	Constellation
	16/32/64/128/256 QAM
	64/256 QAM

	
	DVB-T/T2
	Input Frequency
	60 ~890 MHz

	
	
	Bandwidth
	6/7/8 M

	
	ISDB-T
	Input Frequency
	60 ~890 MHz

	System
	Web management:100M NMS port 

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×328mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤25W (1card inside)
≤50W (2 cards inside)
≤75W (3 cards inside)


 
 
Order Guide
	DX3908-8
	8 FTA DVB-S/S2/S2X Tuner Input, Version 1 or Version 2

	DX3908-16
	16 FTA DVB-S/S2/S2X Tuner Input, Version 1 or Version 2  

	DX3908-24
	24 FTA DVB-S/S2/S2X Tuner Input, Version 1 or Version 2  

	DX3928-8
	8 FTA DVB-C/T/ISDB-T Tuner Input, Version 1 or Version 2

	DX3928-16
	16 FTA DVB-C/T/ISDB-T Tuner Input, Version 1 or Version 2  

	DX3928-24
	24 FTA DVB-C/T/ISDB-TTuner Input, Version 1 or Version 2  


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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