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The FUQ-4213K EIT Multiplexer is a modular head-end device for IP TS conversion, featuring a 1U chassis that supports up to 3 independent cards. Each card processes 512 SPTS or MPTS inputs to 512 SPTS outputs, with CA filter and PSI/SI editing for stream management. It includes web-based configuration and monitoring, ideal for broadcast systems requiring secure and compliant operations. 
Key feature
Enables web-based operation for configuration and monitoring via intuitive interface. 
Specifications
	Input
	512 SPTS or MPTS IP input over UDP, RTP, Unicast and Multicast (per card)

	Output
	512 SPTS IP output UDP, RTP, Unicast and Multicast (per card)

	Multiplexing
	Support CA PID filtering, PID re-mapping

	
	Support accurate PCR adjusting

	
	Support PSI/SI rebuilding and editing

	General
	Dimension(WxLxH)
	482mm×410mm×44mm

	
	Weight
	3.6kg

	
	Temperature
	0~45℃(working )，-20~80℃(storage)

	
	Power supply
	100~240VAC，50/60Hz

	
	consumption
	20W


 
Working Principle (per daughter card)
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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