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The FMUSER FUQ-4214 IP Multiplexer is a high-performance TS processor with 512 IP inputs (SPTS/MPTS) and 2 TS stream outputs. It multiplexes signals, enabling PCR adjusting, PID remapping, and PSI/SI editing. With web-based NMS and front-panel control, it suits digital TV head-end systems and CATV applications. 
Key feature
Supports up to 512 SPTS/MPTS inputs over UDP, compliant with ISO13818 and EN300 468.  
Features dual outputs: 2 ASI groups (each with 2 ports) and 2 IP outputs for reliable transmission.  
Enables advanced processing including PCR adjusting, PID remapping, and PSI/SI editing for up to 2048 PIDs per channel.  
Includes buffer memory for overflow protection, with LCD/keyboard and web-based NMS for easy management.  
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Specifications
	Input
	 IP (RJ45,GE)
	512 x MPTS/SPTS, Unitcast/Multicast, UDP Protocol
IGMP V2/V3

	Re-multiplex
	PID re-mapping (auto or manually available)

	
	PCR accurate adjusting

	
	Automatic generating PSI/SI table

	
	PID passthrough

	
	Support multiplex maximum 2048 PIDs each output channel

	Output port
	 ASI
	2 x independent channels of ASI output (each channel has 2 ports) (up to 210Mbps)

	
	 IP(RJ45,GE)
	 2 x IP (Unitcast/Multicast), UDP Protocol (up to 230Mbps)

	NMS port
	Ethernet port
	GE

	General
	Dimension
	 482mmx410mmx44mm(WxLxH)

	
	Weight
	 2.0kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	 110VAC±10%，50/60Hz; 220VAC±10%，50/60Hz

	
	Consumption
	 <25w


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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