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The FMUSER FUQ-4214 IP Multiplexer processes transport streams with 512 IP inputs (UDP SPTS/MPTS) and delivers 2x2 ASI ports plus 2 IP outputs. It multiplexes programs while inserting EPG, CA, and data services with PSI/SI rebuilding. This 1RU rack-mount unit features web-based NMS and front-panel controls. Ideal for CATV integration and DVB digital headends requiring reliable TS processing.
 
Key feature
- Multiplexes 512 UDP inputs with SPTS/MPTS support and PID remapping (up to 2048 PIDs/channel)
- Delivers 2 independent ASI output groups (4 ports total) + 2 IP outputs over UDP
- Ensures broadcast compliance with ISO13818 & EN300468 including PCR adjustment
- Supports EPG/CA insertion, PSI/SI editing, and huge buffer memory for stability
- Provides web-based NMS, LCD, and keyboard control interfaces
 
Principle Chart
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Specifications
	Input
	 IP (RJ45,GE)
	512 x MPTS/SPTS, Unitcast/Multicast, UDP Protocol
IGMP V2/V3

	Re-multiplex
	PID re-mapping (auto or manually available)

	
	PCR accurate adjusting

	
	Automatic generating PSI/SI table

	
	PID passthrough

	
	Support multiplex maximum 2048 PIDs each output channel

	Output port
	 ASI
	2 x independent channels of ASI output (each channel has 2 ports) (up to 210Mbps)

	
	 IP(RJ45,GE)
	 2 x IP (Unitcast/Multicast), UDP Protocol (up to 230Mbps)

	NMS port
	Ethernet port
	GE

	General
	Dimension
	 482mmx410mmx44mm(WxLxH)

	
	Weight
	 2.0kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	 110VAC±10%，50/60Hz; 220VAC±10%，50/60Hz

	
	Consumption
	 <25w


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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