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The FMUSER FUQ-4313B is a dual-channel audio encoder supporting analog balanced audio and AES/EBU digital audio inputs via XLR interfaces, with outputs for ASI multiplexing and IP/UDP/RTP. It encodes audio signals using MPEG1 Layer 2 and AAC formats. Control is available via LCD/keyboard or Web GUI, featuring hot-pluggable dual/single PSU options. Ideal for digital broadcasting and robust broadcast workflows. 
Key feature
Enables flexible control via LCD/keyboard or Web GUI, with hot-pluggable dual/single PSU options.* MPEG1 Layer 2 and AAC encoding 
Principle Chart
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Specifications
	Input
	Analog balanced audio, XLR interfaces

	
	AES / EBU digital audio, XLR interface

	
	1*ASI input, BNC interface

	Encoding
	Encoding
	MPEG1 Layer 2, AAC

	
	Sample rate
	48KHz

	
	Sample accuracy
	16bit

	
	Bit-rate
	64/96/128/192/256/320/384kbps         

	
	Sound Track
	left, right, stereo (AAC is only for stereo)

	Multiplexing
	Maximum PID Number
	64

	Output
	2 independent ASI outputs, BNC interface (Mirror out of MPTS/SPTS1/SPTS2)

	
	IP output over UDP/RTP protocol, 100M/1000M Self-adaptive rj45 interface (unicast / multicast)

	System function
	LCD/keyboard, Web GUI management
Chinese and English language

	
	Ethernet software upgrade

	General
	Dimensions (W×D×H)
	482mm×350mm×44mm

	
	Temperature range
	0~45℃(operation), -20~80℃(storage)

	
	Power Requirements
	AC 110V±10%,50/60Hz
AC 220V±10%,50/60Hz

	
	Power Consumption
	<15W

	
	Weight
	About 3.2kg


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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