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Product overview
The FMUSER FUQ-4322AB is a professional HD encoder supporting HEVC/H.265 and H.264 video encoding. It accepts inputs from HDMI and HD-SDI sources and outputs via ASI or IP with OSD insertion. Control is managed through web management. Ideal for broadcasting applications like live streaming and television transmission.Multiple audio and video encoding formats are available to meet customers’ various requirements. It supports 2 stereo (4 mono) to mix with the video to form a stream output. The encoded program will finally output in TS through ASI/IP port.
Key feature
- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
- Provides multiple output options including ASI and IP over UDP/RTP/RTSP.  
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- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
- Provides multiple output options including ASI and IP over UDP/RTP/RTSP.  
Specifications
	Video
	Interface
	1×HDMI, 1×HD-SDI

	
	Resolution
	Input
	Output

	
	
	
	MPEG-4 AVC/H.264 HD
	HEVC/H.265 HD

	
	
	1920×1080p@60/59.94
	1920×1080p@60/59.94
	1920×1080p@60/59.94

	
	
	1920×1080p@50
	1920×1080p@50
	1920×1080p@50

	
	
	1920×1080i@60/59.94
	1920×1080i@60
1920×1080p@60/30
	1920×1080p@60

	
	
	1920×1080i @50
	1920×1080i@50
1920×1080p@50/25
	1920×1080p@50

	
	
	1280×720p@60/59.94
	1280×720p@60/59.94
	1280×720p@60/59.94

	
	
	1280×720p@50
	1280×720p@50
	1280×720p@50

	
	Encoding
	HEVC/H.265 HD; MPEG-4 AVC/H.264 HD

	
	Bitrate Range
	HEVC/H.265: 0.5 – 20.00 Mbps
MPEG-4 AVC/H.264: 4 – 20.00 Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IPPP, IBBP

	
	Chroma
	4:2:0

	Audio
	Interface
	2×XLR, 2×AES, 2×RCA, 1×SDI (support maximum 2 stereos synchronous processing), 1×HDMI,

	
	Encoding
	MPEG-1 Layer II, HE-AAC (v1&v2), LC-AAC, DD AC3 passthrough

	
	Sampling rate
	48KHz

	
	Bit-rate
	48Kbps~384Kbps

	Stream Input
	2 ASI Input for remux

	Stream output
	2×ASI output ports, BNC interface

	
	1 IP (MPTS) over UDP / RTP /RTSP, 1000 Base-T Ethernet interface*2 with independent IP addresses (multicast/unicast)

	System function
	LCD/keyboard and web management

	
	Language: English

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×405mm×44.5mm (W × D × H)

	
	Temperature
	0~45℃(Operation), -20~80℃(Storage)

	
	Power
	AC110V±10%, 50/60Hz; AC 220V±10%,50/60Hz

	
	Consumption
	15W


  
- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
- Provides multiple output options including ASI and IP over UDP/RTP/RTSP.  
Technical Comparison
	  
- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
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- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
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- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
- Provides multiple output options including ASI and IP over UDP/RTP/RTSP.  

	FU-4322B
	FU-4322A
	FU-4322HV

	Chipset
	Magnum
	Magnum
	Fujitsu

	Video Encoding
	MPEG-2 HD/SD;
MPEG-4 AVC/H.264 HD/SD
	MPEG-2 HD/SD;
MPEG-4 AVC/H.264 HD/SD
	HEVC/H.265 HD
MPEG-4 AVC/H.264 HD

	Bit Rate
	0.20 – 60.00 Mbps
	0.25Mbps~60.5Mbps
	HEVC/H.265: 0.5 – 20.00 Mbps
MPEG-4 AVC/H.264: 4 – 20.00 Mbps

	HDMI Resolution
	HD
	HD/SD
	HD

	Audio Encode
	MPEG-1 Layer II,
HE-AAC (v1&v2),
LC-AAC,
DD AC3 (2.0),
DD AC3 passthrough (for SDI in)
	MPEG-1 Layer II,
HE-AAC (v1&v2),
LC-AAC;
DD AC3 passthrough
	MPEG-1 Layer II, HE-AAC (v1&v2), LC-AAC,
DD AC3 passthrough (for SDI and HDMI)

	Audio Channel
	Up to 4 stereos
	Up to 2 stereos
	Up to 2 stereos

	Rate Control
	CBR
	CBR/VBR
	CBR/VBR

	Aspect Ratio
	16:9, 4:3, 14:9
	16:9, 4:3, 1:1, 2.35:1
	  
- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
- Offers flexible audio encoding supporting 2 stereos or 4 mono channels with MPEG-1 Layer II, HE-AAC, and LC-AAC.  
- Provides multiple output options including ASI and IP over UDP/RTP/RTSP.  


	Chroma
	4:2:0, 4:2:2
	4:2:0, 4:2:2
	4:2:0

	One-seg
	N/A
	Yes
	N/A

	Video Buffer
	Yes
	N/A
	N/A

	ASI In & Mux
	N/A
	1 ASI input for remux
	2 ASI input for remux

	IP out
	1SPTS over UDP/RTP
	MPTS/8*SPTS over UDP/RTP,
	1 MPTS over UDP / RTP /RTSP

	Low Delay
	150ms, 200ms, 350ms, 650ms
	1400ms - 5000ms, 1ms stepping
	N/A

	Closed Caption
	EIA 608 and EIA 708
	EIA 608 and EIA 708
	EIA 608

	OSD Function
	Yes
	N/A
	Yes

	Management
	Web-server
	Web-server, SNMP
	Web-server


  
- Supports HEVC/H.265 and H.264 HD video encoding with B-frame support.  
- Features OSD insertion for QR codes, logos, and captions.  
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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