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FMUSER FUQ-4322B Professional 4K Encoder Dual HDMI 2.0 Inputs 4 ASI Outputs IP MPTS UDP-RTP H.265 HEVC H.264 Broadcast Streaming
[bookmark: _GoBack][image: 3EEECN_20180703095803]Product Overview
The FMUSER FUQ-4322B is a 4K encoder featuring dual HDMI 2.0 inputs with hot redundancy, supporting H.265/HEVC and H.264/AVC video encoding. It outputs 1 TS via 4 ASI ports and 1 MPTS over IP with real-time bit-rate monitoring. Controlled via web-based NMS, it is ideal for broadcast and streaming applications. 
Key feature
Supports dual HDMI 2.0 inputs with hot redundancy and loop-out for 1080P/4K conversion.  
Encodes video in H.265/HEVC and H.264/AVC formats with CBR control (1–23Mbps).  
Outputs via 4 ASI ports and 1 MPTS over IP (UDP/RTP, unicast/multicast).  
Features broadcast enhancements including logo insertion, captioning, and QR code insertion.  
 (1080P and 4K convert to each other)
 
Specifications
	Input
	1×HDMI input (2.0) with 2 HDMI port, HDCP 2.2/1.4

	
	2 ASI input, BNC interface

	
	32 IP input over UDP and RTP protocol

	Video Input
	Resolution
	Chroma

	
	3840×2160_60P,3840×2160_59.94P, 3840×2160_50P,3840×2160_30P, 3840×2160_29.96P,3840×2160_25P,
3840×2160_24P,1920×1080_60P,
1920×1080_59.94P,1920×1080_50P, 1920×1080_30P ,1920×1080_25P 1920×1080_24P,
	RGB, YCbCr 4:4:4, YCbCr 4:2:2,
YCbCr 4:2:0 (2160P_50/60Hz only)

	Video Encoding
	Encoding
	H.265/HEVC, H.264/AVC

	
	Chroma
	4:2:2, 4:2:0

	
	Bit-rate
	1Mbps~23Mbps

	
	Rate Control
	CBR

	Audio Encoding
	Encoding
	MPEG-1 Layer 2, LC-AAC

	
	Sampling rate
	48KHz

	
	Bit-rate
	64Kbps~256Kbps each channel

	Multiplexing
	2 ASI input multiplexed with local 1 channel of TS

	
	PID remapping (automatically or manually)

	
	Accurate PCR adjusting

	
	Generate PSI/SI table automatically

	Stream output
	1*ASI output through 4 BNC interfaces

	
	1 MPTS over UDP/RTP, 1000M/100M Base-T Ethernet interface (unicast/ multicast)

	System function
	LCD/keyboard operating, web NMS supporting

	
	Ethernet software & hardware upgrade

	Miscellaneous
	Dimension (W× L× H)
	482mm×455mm×44mm

	
	Approx weight 
	4kg

	
	Temperature
	0~45℃(work),  -20~80℃（Storage）

	
	Power
	AC 100V-220V±10%, 50/60Hz

	
	Consumption
	25W


 
Principle Chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.

   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image2.jpeg
;oW Encod

Upgrade

FOMNE HOM N2





image3.jpeg
H.265/H.264

Encoding

B ASI Output

ASI Inl
ASI In2




image1.png
FMuser




