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Product overview
The FUQ-4322C HD encoder supports MPEG-2 and H.264 encoding, with inputs including HDMI, SDI, YPbPr, CVBS for video and AES, BNC, XLR for audio, and outputs TS streams via ASI or IP. It processes signals by encoding them with OSD insertion for QR codes, logos, and captions. The device features LCD/keyboard and web management interfaces for control. Ideal for broadcast applications such as television broadcasting and network integration. 
Key feature
Supports MPEG-2 and H.264 video encoding for resolutions like 1080i/p and 720p.  
Encodes audio in MPEG-1 Layer II, HE-AAC, LC-AAC, and DD AC3 formats with passthrough.  
Enables OSD insertion of QR codes, logos, and captions during encoding.  
Delivers streams via ASI output and IP over UDP/RTP for MPTS distribution.  
Features LCD/keyboard and web management interfaces for configuration.   
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Specifications
	[bookmark: OLE_LINK1]Video
	Interface
	1×HDMI, 1×HD-SDI, 1×YPbPr and 1×CVBS (only for CC)

	
	Resolution
	Input
	Output
	Interface Applicable

	
	
	1920×1080p@60/59.94
	1920×1080p@60,
	SDI, HDMI

	
	
	1920×1080p@50
	1920×1080p@50
	

	
	
	1920×1080i@60/59.94
	1920×1080i @60
	SDI, HDMI, YpbPr

	
	
	1920×1080i @50
	1920×1080i @50
	

	
	
	1280×720p@60/59.94
	     1280×720p@60
	

	
	
	1280×720p@50
	     1280×720p@50
	

	
	
	720×576i@50
	720×576i @50
	SDI, HDMI

	
	
	720×480i@60
	720×480i @60
	

	
	Encoding
	MPEG-2 HD/SD,
MPEG-4 AVC/H.264 HD/SD

	
	Bitrate Range
	2.5 – 19.00 Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP, IBBP, IBBBP

	
	Chroma
	4:2:0

	Audio
	Interface
	2×XLR, 2×AES, 2×BNC, 1×SDI (support maximum 2 stereos synchronous processing), 1×HDMI,

	
	Encoding
	MPEG-1 Layer II, HE-AAC (v1&v2), LC-AAC, DD AC3 (2.0)
DD AC3 pass-through (for SDI and HDMI in)

	
	Sampling rate
	48KHz

	
	Bit-rate
	32Kbps~384Kbps

	Stream Input
	2 ASI Input for remux

	Stream output
	2×ASI output ports, BNC interface

	
	2 IP (MPTS) over UDP / RTP /RTSP, 1000 Base-T Ethernet interface*2 with independent IP addresses (multicast/unicast)

	System function
	LCD/keyboard and web management 

	
	Language: English

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×405mm×44.5mm (W × D × H)

	
	Temperature
	0~45℃(Operation), -20~80℃(Storage)

	
	Power
	AC110V±10%, 50/60Hz; AC 220V±10%,50/60Hz

	
	Consumption
	16W


 
Technical Comparison
	 
	FU-4322B(V2)
	FU-4322HS

	Chipset
	Vixs
	Hisilicon

	Video Encoding
	MPEG-2 HD/SD;
MPEG-4 AVC/H.264 HD/SD
	HEVC/H.265 HD/SD
MPEG-4 AVC/H.264 HD/SD

	Bit Rate
	2.5Mbps~19.0Mbps
	1Mbps~15Mbps

	HDMI Resolution
	HD/SD
	HD/SD

	Audio Encode
	MPEG-1 Layer II, 
HE-AAC (v1&v2), 
LC-AAC,
DD AC3 (2.0),
DD AC3 pass-through (for SDI and HDMI in)
	MPEG-1 Layer II, HE-AAC (v1&v2), LC-AAC,
DD AC3 pass-through (for SDI and HDMI in)

	Audio Channel
	Up to 2 stereos
	Up to 2 stereos

	Rate Control
	CBR/VBR
	CBR/VBR

	Aspect Ratio
	16:9, 4:3
	 

	Chroma
	4:2:0
	4:2:0

	Video Buffer
	Yes
	N/A

	ASI In & Mux
	2 ASI input for remux
	2 ASI input for remux

	IP out
	1 MPTS over UDP / RTP /RTSP
	1 MPTS over UDP / RTP /RTSP

	Low Delay
	150ms - 650ms
	N/A

	Closed Caption
	EIA 608 and EIA 708
	EIA 608


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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