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Product Overview
The FMUSER FUQ-4337SB is a multi-channel SD encoder supporting up to 48 CVBS inputs, with MPEG4 AVC/H.264 video encoding and outputs MPTS and SPTS via IP and ASI interfaces. It processes SD video signals for digital distribution, housed in a modular 1U chassis allowing up to three standalone modules with web-based management. Ideal for digital TV distribution systems like CATV and satellite headends.
 
Key feature
Supports 16/32/48× CVBS inputs with MPEG4 AVC/H.264 SD video encoding for PAL and NTSC formats.  
Features MPEG-1 Layer II audio encoding with adjustable gain and multiple bit-rate options.  
Provides MPTS output via ASI and SPTS output over IP with UDP/RTP support, including Null PKT Filter.  
Supports logo, caption, and QR code insertion for customized content.  
Modular 1U chassis design allows up to 3 standalone modules with web-based management for real-time monitoring and easy updates.
 
Principle Chart
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Technical specification
	[bookmark: OLE_LINK1]Input
	16/32/48 CVBS inputs , DB15-To-RCA interface

	Video
	Resolution
	[bookmark: OLE_LINK8]720×576i (PAL-B,D,G,H,I), 720×480i (NTSC-M,J)

	
	Encoding
	MPEG4 AVC/H.264(HP/MP/BP)

	
	Bit-rate
	1Mbps~66Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	[bookmark: OLE_LINK13]IPP (P frame is adjustable)

	
	Aspect Ratio
	4:3; 16:9

	Audio
	Encoding
	MPEG-1 Layer 2

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 adjustable

	
	Bit-rate
	64/128/192/224/256/320/384Kbps each channel

	Stream output
	[bookmark: OLE_LINK23]IP (1*MPTS and 16*SPTS for one module) output over UDP and RTP, 1000 Base-T Ethernet interface (Multicast and unicast)

	
	1 MPTS output through 1 ASI output ports, BNC interface (Optional)

	System function
	Network management (WEB)

	
	English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
 
Order Information
	 
	Version I
	Version II
	Version III

	16 CVBS Input
	○
	 
	 

	32 CVBS Input
	 
	○
	 

	48 CVBS Input
	 
	 
	○


 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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