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Product Overview
[bookmark: OLE_LINK12]The FMUSER FUQ-4339K-N (V2) is a network encoder with 48 HDMI inputs and IP outputs. It encodes video in HEVC/H.265 and MPEG-4 AVC/H.264 formats, and audio in MPEG-1 Layer 2, LC-AAC, HE-AAC, with AC3 Pass Through. This 2-U rack-mountable device streams via UDP, SRT, RTSP, RTMP, HTTP, and HLS. Ideal for IP broadcasting in studios and streaming services. 
[bookmark: OLE_LINK10]Key feature
- Features 48 HDMI inputs configurable via six encoder modules for SPTS output.  
- Supports HEVC/H.265 and MPEG-4 AVC/H.264 video encoding.  
- Offers flexible audio options including MPEG-1 Layer 2, LC-AAC, HE-AAC, and AC3 Pass Through.  
- Provides multi-protocol IP output via UDP, SRT, RTSP, RTMP, HTTP, and HLS.  
- Enables enhanced features like QR code, LOGO, and caption insertion.  
Inner Principle Chart (Per 8-HDMI Module)
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Specifications
	[bookmark: OLE_LINK1]Input
	48 HDMI inputs

	Video
	Resolution
	input
	1920×1080_60P, 1920×1080_60i,
1920×1080_50P, 1920×1080_50i,
1280×720_60P, 1280×720_50P,
720 x 576_50i,720 x 480_60i

	
	
	[bookmark: OLE_LINK9]Output
	1920×1080_30P, 1920×1080_25P,
1280×720_30P, 1280×720_25P,
720 x 576_25P, 720 x 480_30P

	
	Encoding
	HEVC/H.265 HD/SD; MPEG-4 AVC/H.264 HD/SD

	
	Bit-rate
	1~13Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP…P (P Frame adjustment, without B Frame )

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass through

	
	Sampling rate
	32KHz, 48KHz, 44.1KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	LC-AAC Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC Bit-rate
	48/56/64/80/96/112/128 kbps

	Stream output
	[bookmark: OLE_LINK24]IP out over UDP (Unicast/Multicast),SRT, RTP,RTSP, RTMP, HTTP, HLS (RJ45, 1000M ) (8 HDMI inputs with 8 SPTS for each encoder board)

	System function
	Network management(WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×88mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
Major spec comparison
	　
	FU-4339S-N
	FU-4339M-N v1
	FU-4339M-N v2

	HDMI Channel
	8/16/24
	2/4/8/16/24
	48

	Video Format
	H.264
	H.264/H.265
	H.264/H.265

	Resolution
	HD/SD
	HD
	HD/SD

	OSD
	Yes
	No
	Yes

	Chassis
	1-U
	1-U
	2-U


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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