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The FUQ-4339R Encoder is a professional HD/SD audio and video encoding device with scalable 8/16/24 HDMI inputs and outputs including 1 MPTS and 8 SPTS per module. It processes signals using MPEG4 AVC/H.264 video encoding and MPEG1 Layer II, LC-AAC, HE-AAC audio formats. Controlled via web management, it supports features like QR code and caption insertion. Ideal for cable TV head-ends and broadcasting systems. 
Key feature
Supports scalable 8/16/24 HDMI inputs with 1 MPTS and 8 SPTS outputs per module.
Features H.264 video encoding and MPEG audio formats including LC-AAC and HE-AAC.
Provides IP output over UDP/RTP/RTSP and optional ASI output.
Includes web management for control with QR code and caption insertion support.
Supports Null Packet Filter for stream optimization.
 
Principle Chart (Each Encoder Module)
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Technical specification
	Input
	8/16/24 HDMI inputs

	Video
	Resolution
	input
	1920×1080_60P, 1920×1080_60i,
1920×1080_50P, 1920×1080_50i,
1280×720_60P, 1280×720_50P,
720 x 576_50i,720 x 480_60i

	
	
	Output
	1920×1080_30P, 1920×1080_25P,
1280×720_30P, 1280×720_25P,
720 x 576_25P, 720 x 480_30P

	
	Encoding
	MPEG-4 AVC/H.264

	
	Bit-rate
	1~13Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP…P (P Frame adjustment, without B Frame )

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass through

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2 Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	 
	LC-AAC Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC Bit-rate
	48/56/64/80/96/112/128 kbps

	Stream output
	IP output through DATA (GE) over UDP and RTP/RTSP protocol
(8 HDMI inputs with 8 SPTS and 1MPTS output for each encoder board)
1 ASI out as mirror of MPTS (Optional as order)

	System function
	Network management(WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
Order Information
	 
	FU-4339S-8
	FU-4339S-16
	FU-4339S-24

	8 HDMI Inputs with 8 SPTS and 1 MPTS out (1 encoder board+1NMS port+1 DATA Port)
	X
	 
	 

	16 HDMI Inputs with 16 SPTS or 2 MPTS out (2 encoder boards+2 NMS ports+2 DATA Ports)
	 
	X
	 

	24 HDMI Inputs with 24 SPTS or 3 MPTS out((3 encoder boards+3 NMS ports+ 3 DATA Ports))
	 
	 
	X


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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