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Product Overview
[bookmark: OLE_LINK13]The FMUSER FUQ-4339R-N is a multi-channel network encoder with up to 24 HDMI inputs, supporting H.264 video and AAC audio encoding for IP broadcasting. It processes signals by encoding and streaming via protocols like UDP, SRT, RTMP, and HLS over internet/LAN. Featuring web-based management for control and updates. Ideal for applications in live event streaming to PCs, smartphones, and mobile devices. 
Key feature
  
- Supports up to 24 HDMI inputs with individual SPTS output for flexible channel configuration.  
- Features MPEG-4 AVC/H.264 video encoding and AAC audio encoding including LC-AAC, HE-AAC, and AC3 pass-through.  
- Enables multiple IP output protocols: UDP (Unicast/Multicast), SRT, RTSP, RTMP, HTTP, and HLS for versatile streaming.  
- Offers caption, logo, and QR code insertion with multi-language capabilities for content customization.  
- Provides web-based management for easy control, updates, and network administration.   
Inner Principle Chart (Per Module)
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Specifications 
	[bookmark: OLE_LINK1]Input
	8/16/24 HDMI inputs 

	Video
	Resolution
	input
	1920×1080_60P, 1920×1080_60i,
1920×1080_50P, 1920×1080_50i,
1280×720_60P, 1280×720_50P, 
720 x 576_50i,720 x 480_60i

	
	
	[bookmark: OLE_LINK9]Output
	1920×1080_30P, 1920×1080_25P,
1280×720_30P, 1280×720_25P, 
720 x 576_25P, 720 x 480_30P

	
	Encoding
	MPEG-4 AVC/H.264

	
	Bit-rate
	1~13Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP…P (P Frame adjustment, without B Frame )

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass through

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2 Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	LC-AAC Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC Bit-rate
	48/56/64/80/96/112/128 kbps

	Stream output
	[bookmark: OLE_LINK24]IP out over UDP (Unicast/Multicast),SRT, RTP,RTSP, RTMP, HTTP, HLS (RJ45, 1000M ) (8 HDMI inputs with 8 SPTS for each encoder board) 

	System function
	Network management(WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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