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Product Overview
The FMUSER FUQ-433X-Y is a multi-channel network encoder with 24 HDMI inputs and IP streaming output via RJ45. It encodes video using H.265/HEVC or H.264/MPEG-4 AVC compression and streams via protocols like UDP, SRT, RTMP, and HLS. Managed through a web-based interface, it supports remote configuration and software upgrades. Ideal for IP broadcasting to PCs, smartphones, and mobile devices in live streaming and broadcast applications. 
Key feature
Supports 24 HDMI inputs with individual SPTS output, handling resolutions up to 1920×1080 at 60P/50P.  
Features H.265/HEVC and H.264/MPEG-4 AVC encoding with 1–7 Mbps bitrate, CBR/VBR control, and IP GOP structure.  
Enables multi-protocol streaming via UDP (Unicast/Multicast), SRT, RTSP, RTMP, HTTP, and HLS over 1000M RJ45.  
Provides flexible audio encoding with MPEG-1 Layer 2, LC-AAC, and HE-AAC, supporting 32–48 kHz sampling and adjustable gain.  
Inner Principle Chart (Per Module)
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Specifications
	Input
	2/4/8/16/24 HDMI inputs

	Video
	Resolution
	1920*1080_60P, 1920*1080_50P; 1920*1080_59.94P, 1280*720_60p,
1280*720_59.94, 1280*720_50P

	
	Encoding
	H.264/H.265

	
	Bit-rate
	1~7Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass through

	
	Sampling rate
	32KHz,44.1KHz,48KHz

	
	Chroma
	4:2:0

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	LC-AAC Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC Bit-rate
	48/56/64/80/96/112/128 kbps

	Stream output
	IP out over UDP (Unicast/Multicast), SRT, RTP,RTSP, RTMP, HTTP, HLS (RJ45, 1000M) (8 HDMI inputs with 8 SPTS for each encoder board)

	System function
	Network management(WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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