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The FMUSER FUQ-4347X/FUQ-4355X encoder provides high-density HDMI encoding with 16 or 24 HDMI inputs and outputs 1 MPTS plus 8 SPTS per module. It encodes video using MPEG4 AVC/H.264 and audio with MPEG1 Layer II, LC-AAC, or HE-AAC, supporting AC3 Pass Through. The device offers web-based management for control and customization, including QR code/LOGO/caption insertion and "Null PKT Filter" support. Ideal for digital headends, cable TV systems, and broadcasting applications. 
Key feature  
· - Supports 16 or 24 HDMI inputs with SPTS/MPTS output per module.  
· - Encodes video in MPEG4 AVC/H.264 and audio in MPEG1 Layer II, LC-AAC, HE-AAC with AC3 Pass Through.  
· - Streams via UDP/RTP/RTSP protocols over GE DATA port.  
· - Features web management for updates, QR code/LOGO/caption insertion, and "Null PKT Filter" support.  
· MPEG4 AVC/H.264 video encoding format
· MPEG1 Layer II, LC-AAC，HE-AAC audio encoding format and AC3 Pass Through, and audio gain adjustment
· IP output over UDP and RTP/RTSP protocol
· Support QR code, LOGO, caption insertion
· Support “Null PKT Filter” function
· Control via web management, and easy updates via web
 
Principle Chart (Each Encoder Module)
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Technical specification
	Input
	16 HDMI inputs (FU-4347S); 24 HDMI inputs (FU-4355S)

	Video
	Resolution
	input
	1920×1080_60P, 1920×1080_60i,
1920×1080_50P, 1920×1080_50i,
1280×720_60P, 1280×720_50P, 
720 x 576_50i,720 x 480_60i

	
	
	Output
	1920×1080_30P, 1920×1080_25P,
1280×720_30P, 1280×720_25P, 
720 x 576_25P, 720 x 480_30P

	
	Encoding
	MPEG-4 AVC/H.264

	
	Bit-rate
	1~13Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP…P (P Frame adjustment, without B Frame )

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass through

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2 Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	LC-AAC Bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC Bit-rate
	48/56/64/80/96/112/128 kbps

	Stream output
	IP output through DATA (GE) over UDP and RTP/RTSP protocol
(8 HDMI inputs with 8 SPTS and 1MPTS output for each encoder module) 

	System function
	Network management (WEB)

	
	English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	440mm×324mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
Order Guide
	P/N
	Config

	FU-4347S
	16 HDMI inputs

	FU-4355S
	24 HDMI inputs



 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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