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Product Overview
The FMUSER FUQ-4349S is an 8-in-1 FM receiver that captures FM audio and outputs via ASI and IP ports. It compresses audio into digital TS streams using MPEG1 Layer 2 encoding. Features LCD/keyboard control and web-based NMS for management. Ideal for professional audio distribution in HFC or terrestrial systems, integrating with STBs or TVs.Each antenna receives two audios and this unit can maximally process 8 audios. In addition, it is equipped with one ASI input port as well for Audio/Video re-mux. It is featured to operators with its high capacity and integration.
 
Key feature
Supports reception of 8 FM audio channels via 4 antennas for dual-audio capability.  
Features ASI input for Audio/Video re-mux and remultiplexing.  
Provides MPEG1 Layer 2 audio encoding with adjustable bit-rates and volume control.  
Offers 2 ASI mirrored outputs and IP output over UDP/RTP for versatile distribution.  
Enables control via LCD/keyboard and web-based NMS for monitoring and updates.
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Specifications
	FM Receiving
	Antenna Frequency
	76-108 MHz

	
	Volume Control
	0%-100%

	
	FM lock status and signal quality display

	Audio Encode
	Encoding Format
	MPEG1 Layer 2

	
	Audio Gain
	0-255

	
	Sampling Rate
	48KHz

	
	Bit-rate
	32/48/56/64/80/96/112/128/160/192/224/256/320/384Kb/s (each channel)

	Stream In/Out
	1*ASI input, BNC interface

	
	2*ASI mirrored output, BNC interface

	
	8*SPTS+1*MPTS over UDP/RTP, 1000M Base-T Ethernet interface (unicast/multicast) (SPTS output is for the FM input audio)

	System
	LCD/keyboard operating, web-based NMS manage

	
	Language: English/Chinese

	
	Ethernet software & hardware upgrade

	Miscellaneous
	Dimension
	482mm×455mm×44mm (W× L× H)

	
	Temperature
	0~45℃ (work),  -20~80℃（Storage）

	
	Power
	AC 100V-220V±10%, 50/60Hz


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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