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The FMUSER FUQ-4353 is a dual-channel encoder supporting HD/SD MPEG-2 & H.264 video and MP2/AAC/AC3 audio. It accepts pluggable HDMI/3G-SDI/YPbPr+CVBS inputs and delivers ASI re-muxed outputs (MPTS/SPTS) or IP streams (UDP/RTP). The 1RU rack-mount unit features PSI/SI editing and web-based NMS for broadcast and IPTV workflows.
Key feature
Centralized Control: Web GUI and SNMP v2 for remote management via network 
Technical Specifications
	HDMI Input
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	Video
	Input
	HDMI*1 (with one for backup)

	
	
	Encoding
	MPEG2; MPEG4 AVC/H.264

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	1920*1080_60P, 1920*1080_50P,
(-for MPEG4 AVC/H.264 only)
1920*1080_60i, 1920*1080_50i,
1280*720_60p, 1280*720_50P
720*480_60i, 720*576_50i

	
	
	Low Delay
	Normal, Mode 1, Mode 2

	
	
	Chroma
	4:2:0

	
	
	Aspect Ratio
	16:9,4:3

	
	Audio
	 
Encoding
	MPEG1 Layer II;MPEG 2-AAC; MPEG 4-AAC and Dolby Digital AC3 2.0

	
	
	Sample rate
	48KHz

	
	
	Bitrate
	64/96/128/ 192/256/320kbps

	 

	HDMI/YPbPr/CVBS 3-in-1 Input
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(under developing)
	Video
(HDMI)
	Encoding
	MPEG2; MPEG4 AVC/H.264

	
	
	Input
	HDMI*1

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	1920*1080_60P, 1920*1080_50P,  
-for MPEG4 AVC/H.264 only)
1920*1080_60i, 1920*1080_50i,
1280*720_60p, 1280*720_50P
720*480_60i, 720*576_50i

	
	
	Low Delay
	Normal, Mode 1, Mode 2

	
	
	Chroma
	4:2:0

	
	
	Aspect Ratio
	16:9,4:3

	
	Audio
(HDMI)
	Encoding
	MPEG1 Layer II ,MPEG2-AAC, MPEG4-AAC
and Dolby Digital AC3 2.0

	
	
	Input
	HDMI*1

	
	
	Sample rate
	48KHz

	
	
	Bitrate
	64/96/128/ 192/256/320kbps

	
	Video
(YpbPr/ CVBS)
	Encoding
	MPEG2; MPEG4 AVC/H.264

	
	
	Input
	YpbPr*1 / CVBS *1

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	CVBS: 720x576_50i (PAL); 720x480_60i (NTSC)
YpbPr: 1920*1080_60i, 1920*1080_50i;
1280*720_60p, 1280*720_50P

	
	
	Low Delay
	Normal, Mode 1, Mode 2

	
	
	Chroma
	4:2:0

	
	
	Aspect Ratio
	16:9, 4:3

	
	Audio
(YpbPr/ CVBS)
	Encoding
	MPEG1 Layer II; MPEG2-AAC; MPEG4-AAC
and Dolby Digital AC3 2.0

	
	
	Interface
	1*Stereo/2*mono

	
	
	Sample rate
	48KHz

	
	
	Bit rate
	64/96/128/ 192/256/320kbps

		SDI Input
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	Video
	Encoding
	MPEG2; MPEG4 AVC/H.264

	
	
	Input
	SDI*1

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only)
1920*1080_60i, 1920*1080_50i,
1280*720_60p, 1280*720_50P
720*480_60i, 720*576_50i

	
	
	Low Delay
	Normal, Mode 1, Mode 2

	
	
	Chroma
	4:2:0

	
	
	Aspect Ratio
	16:9,4:3

	
	Audio
	Encoding
	MPEG1 Layer II ,MPEG2-AAC, MPEG4-AAC
and Dolby Digital AC3 2.0

	
	
	Sample rate
	48KHz

	
	
	Bitrate            
	64/96/128/ 192/256/320kbps





 
	General
	System
	Local interface
	LCD + control buttons

	
	
	Remote management
	Web NMS

	
	
	Stream In
	1 ASI in for re-multiplexing

	
	
	Stream Out
	2 ASI out (BNC type, same one TS, mirror as MPTS or SPTS)

	
	
	
	IP (1 MPTS & 2 SPTS) over UDP, RTP/RTSP (RJ45, 1000M)

	
	
	DATA Port
	1000M

	
	
	NMS interface
	RJ45, 100M

	
	
	Language
	English

	
	Physical Specification
	Power supply
	100~240VAC, 50/60Hz

	
	
	Dimensions
	482*300*44mm

	
	
	Operation temp
	0~45℃


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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