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The FMUSER FUQ-4353B is a professional HD/SD encoder supporting MPEG-2 and H.264 video encoding with four SDI or HDMI inputs. It processes signals by encoding and re-multiplexing into MPTS or SPTS, outputting via ASI and IP. Featuring a modular drawer design, it is ideal for broadcast, cable TV, and streaming applications.HDMI inputs supporting MPEG‐2 and MPEG‐4 AVC/H.264 video encoding and
MPEG 2, MPEG 2‐AAC, MPEG 4‐AAC and DD AC3 audio encoding. The 4 encoded programs will output through ASI and IP ports in MPTS or SPTS, and there is also one ASI in port for re-multiplexing.
It adopts inner drawer‐type structural design which greatly facilitates the change of encoding modules if needed.
 
Key feature
Supports MPEG2 HD/SD and MPEG4 AVC/H.264 video encoding with resolution downscale conversion  
Multiple audio encoding options: MPEG2, AAC, and AC3, including dialog normalization  
Flexible input configurations: 4x SDI, 4x HDMI, or mixed inputs  
Advanced features: low delay, closed caption support, and web-based NMS management  
 
Principle Chart
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Technical Specifications
Encoding Section
Video
	Encoding
	MPEG2 & MPEG4 AVC/H.264

	Input
	SDI*4 or HDMI*4 + 1 ASI in

	Resolution
	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only)
1920*1080_60i, 1920*1080_50i,
1280*720_60p, 1280*720_50P
720*480_60i, 720*576_50i

	Support object resolution 
(for downscale conversion)
	1920*1080_60P, 1920*1080_50P, (-for MPEG4 AVC/H.264 only)
1440*1080_60i, 1440*1080_50i,
1280*720_60p, 1280*720_50P
720*480_60i, 720*576_50i

	Bit Rate
	1~19.5Mbps

	Chroma Sample
	4:2:0

	Aspect Ratio
	16:9, 4:3


Audio
	encoding
	MPEG 2, MPEG2-AAC, MPEG4-AAC, Dolby Digital AC3 (2.0)

	Dialog Normalization
Applicable for DD AC3 encoding only)
	-31 ~ -1 dB

	Sample rate
	48KHz

	Bit rate
	64kbps, 96kbps,128kbps, 192kbps, 256kbps, 320kbps


 
System
	Local interface
	LCD + control buttons

	Remote management 
	Web NMS

	Low Delay Mode
	Normal, mode 1, mode 2, Manual

	output
	2*ASI out (BNC type, mirror ports/the same one TS);
IP (1 MPTS & 4 SPTS) over UDP, RTP/RTSP (RJ45, 1000M)

	NMS interface
	RJ45, 100M

	Language
	English


 
General
	Power
	AC 100V~240V

	Dimensions
	482*400*44mm

	Operation temperature
	0~45℃


 
 
Technical Comparision
	 
	The Former Version
	The Current Version（V2）

	ASI in
	No
	Yes

	Bit rate Mode
	CBR/VBR option
	CBR

	Audio Group/Pair option-SDI
	No
	Yes

	Video Bit Rate
	0.5~19.5Mbps for H.264 encoding
1~19.5Mbps for MPEG-2 encoding
	1~19.5Mbps

	Low Delay
	Normal/Mode 1/Mode 2
	Normal/Mode 1/Mode 2/Manual

	Character Encoding option
	No
	Yes

	Output Protocol
	UDP, RTP
	UDP, RTP/RTSP

	DATA Port
	100M port
	1000M port


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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