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The FMUSER FUQ-4353C is a professional 4-in-1 HD encoder featuring 4x HDMI/YPbPr/CVBS inputs and dual-output via ASI (2x) + IP (UDP/RTP/RTSP). It performs real-time MPEG2/MPEG4 H.264 encoding with AC3 passthrough and EIA608 Closed Captioning support. The 1RU rack-mount unit offers web-based NMS control and firmware upgrades. Ideal for digital TV headends, IPTV systems, and satellite uplink applications.
Key feature
1. Multi-standard encoding: Supports MPEG2 & H.264 with HD-to-SD downscaling (1080i/720p/576i)  
2. Flexible audio handling: AC3 2.0/5.1/7.1 passthrough + MPEG4-AAC/MP2 encoding  
3. Dual-output architecture: 2x ASI outputs (SPTS/MPTS) + IP streaming (UDP/RTP/RTSP)  
4. Broadcast features: EIA608 Closed Captioning, LCN support, low-latency mode  
5. Remote management: Web GUI + SNMP v2/v3 for NMS integration
Principle Chart
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Specifications
	Encoding Section

	Video (HDMI)

	Encoding
	MPEG2; MPEG4 AVC/H.264

	Interface
	HDMI*4

	Resolution
	Input
	Output

	
	1920*1080_60P, 1920*1080_50P
(For MPEG 4 AVC/H.264 only),
1920*1080_60i, 1920*1080_50i,
1280*720_60p, 1280*720_50P
	1920*1080_60i, 1920*1080_50i,
1440*1080_60i, 1440*1080_50i
1280*720_60p, 1280*720_50P,
720*480_60i, 720*576_50i

	Low Delay
	Normal, Mode 1, Mode 2

	Audio (HDMI)

	Encoding
	MPEG1 Layer II; MPEG2-AAC; MPEG4-AAC;
DD AC3 (2.0) Optional;
DD AC3 (2.0/5.1/7.1) passthrough

	Interface
	HDMI*4 /SPDIF*4

	Sample rate
	48KHz

	Bit rate
	64/96/128/ 192/256/320kbps

	Video (CVBS/YPbPr)

	Encoding
	MPEG2; MPEG4 AVC/H.264

	Interface
	CVBS/YPbPr*4 (RCA)

	Resolution
	CVBS: 720*576_50i, 720*480_60i

	
	YPbPr Input
	YPbPr Output

	
	 
1920*1080_60i, 1920*1080_50i;
1280*720_60p, 1280*720_50P
	1920*1080_60i, 1920*1080_50i,
1440*1080_60i, 1440*1080_50i
1280*720_60p, 1280*720_50P,
720*480_60i, 720*576_50i

	Low Delay
	Normal, Mode 1, Mode 2

	Audio (L/R)

	Encoding
	MPEG1 Layer II; MPEG2-AAC; MPEG4-AAC;
DD AC3 (2.0) Optional

	Interface
	4*Stereo/8*mono/4*SPDIF

	Sample rate
	48KHz

	Bit rate
	64/96/128/ 192/256/320kbps


 
	System

	Local interface 
	LCD + control buttons

	Remote management
	Web NMS

	Stream Out
	2 ASI mirrored out (BNC type, 100M);
IP (MPTS&4 SPTS) over UDP, RTP/RTSP out (RJ45, 100M)

	NMS interface
	RJ45, 100M

	Aspect Ratio
	4:3; 16:9

	Language
	English

	General

	Power supply
	AC 100V~240V

	Dimensions
	482*400*44mm

	Weight
	4.5 kg

	Operation  temperature
	0~45℃


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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