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The FUQ-4354 integrates demodulation, descrambling, decoding, and transcoding, supporting inputs like 32× IP, 2× tuner, and 1× ASI, with outputs including IP, ASI, CVBS, YPbPr, HDMI, and SDI. It processes signals by converting AVS+ to H.264/MPEG-2, transcoding video and audio, and downscaling HD to SD. Managed via web-based NMS, it is designed for broadcast systems, enabling efficient video handling for operators.It can be easily managed through web NMS system, and has become an ideal solution for operator to provide high quality video trans-coding.
 
KeyFeature
- Supports multi-format inputs: 32× IP (UDP/RTP), 2× tuner with CAM/CI slots, and 1× ASI.
- Enables flexible transcoding: AVS+/MPEG-2/H.264 SD/HD video conversion; MPEG-2/AAC/AC3 audio with CBR/VBR control.
- Provides diverse outputs: IP/ASI streams, CVBS, YPbPr, HDMI, and SDI.
- Features advanced control: BISS descrambling, web-based NMS, and local LCD/keyboard management.
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Specifications
 
	Stream In
	32 IP over UDP/RTP, 2*100/1000M Base-T Ethernet Interface

	
	2 * DVB-C/T/S2/ATSC Tuners

	
	1 ASI input

	BISS Descramble
	1 program

	
	Mode 0, Mode1, Mode E

	Transcoding 
	Video
	AVS+ HD → MPEG2/H.264 HD
AVS+ HD → MPEG2/H.264 SD
AVS+ SD → MPEG2/H.264 SD

	
	
	MPEG2 HD → MPEG2/H.264 HD ;
MPEG2 HD → MPEG2/H.264 SD ;
MPEG2 SD → MPEG2/H.264 SD

	
	
	H.264 HD → MPEG2/H.264 HD ;
H.264 HD → MPEG2/H.264 SD ;
H.264 SD → MPEG2/H.264 SD

	
	Audio
	MPEG-2, MPEG-2 AAC, MPEG-4 AAC and AC3 any to any; AC3 pass through

	Decoding
	Video Output
	1×CVBS; 1×YPbPr ; 1×HDMI; 2×HD-SDI

	
	Resolution
	480i，480p，576i，576p，720p@50，720p@60，1080i@50，1080i@60, 1080p@50, 1080p@60

	
	Rate Control
	CBR/VBR  

	
	Audio Output
	1*Stereo /2*mono, HDMI，SDI

	
	Audio Sampling
	48KHz  

	
	Audio Bit Rate
	64Kbps-384Kbps  

	Stream Out
	3*IP over UDP protocol, 2*100M/1000M Base-T Ethernet Interface, one for backup

	
	2 groups separate ASI outputs (each group has 2 channels, as a copy of one of IP) output, BNC interface

	System Function 
	LCD & Key board control; web-based NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm (WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 200V-240V, 50/60Hz, 2A


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.

   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image4.jpeg
AVS+HD MPEG2/H.264 HD MPEG 1 Layer 2 MPEG-4 AAC

AVS+ SD MPEG2/H.264 SD
MPEG-2 AAC AC3

MPEG2SD H.264 SD
f AC3

MPEG2 HD H.264 HD Passthrough




image2.jpeg
—— ) Asw

@@ e





image3.jpeg
CVBS/YPbPr/HDMI/SD]

Gl —
a—: !

IP (MPTS)

32 *IP (MPTS/SPT.

1*ASI ’

2*Tuner ’ ASI 1(as mirror of one IP

ASI 2(as mirror of one IP




image1.png
FMuser




