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The FMUSER FUQ-4354 is a single-channel transcoder integrating demodulation (optional DVB-C/T/S2/ATSC), descrambling, decoding, and transcoding. It processes signals by accepting inputs via 2 tuners with CAM/CI slots, ASI, and 32 IP streams (UDP/RTP), supporting any-to-any conversion between AVS+ and H.264/MPEG-2 with HD-to-SD downscaling. Controlled via web NMS, this unit is ideal for broadcast transmission and cable distribution systems. 
KeyFeature
Supports flexible inputs: 32 IP streams (UDP/RTP), 2 tuners with CAM/CI slots, and ASI.
Enables multi-format video transcoding: any-to-any conversion between AVS+, MPEG-2, and H.264 in SD/HD, including HD-to-SD downscaling.
Features advanced audio handling: any-to-any transcoding of MPEG-2, AAC, and AC3 with AC3 pass-through.
Provides robust outputs: 3 IP (UDP), 2 ASI groups, and decoded video/audio (CVBS/YPbPr/HDMI/SDI).
Offers secure management: BISS descrambling, CBR/VBR control, and web NMS for remote monitoring.
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Specifications
 
	Stream In
	32 IP over UDP/RTP, 2*100/1000M Base-T Ethernet Interface

	
	2 * DVB-C/T/S2/ATSC Tuners

	
	1 ASI input

	BISS Descramble
	1 program

	
	Mode 0, Mode1, Mode E

	Transcoding 
	Video
	AVS+ HD → MPEG2/H.264 HD
AVS+ HD → MPEG2/H.264 SD
AVS+ SD → MPEG2/H.264 SD

	
	
	MPEG2 HD → MPEG2/H.264 HD ;
MPEG2 HD → MPEG2/H.264 SD ;
MPEG2 SD → MPEG2/H.264 SD

	
	
	H.264 HD → MPEG2/H.264 HD ;
H.264 HD → MPEG2/H.264 SD ;
H.264 SD → MPEG2/H.264 SD

	
	Audio
	MPEG-2, MPEG-2 AAC, MPEG-4 AAC and AC3 any to any; AC3 pass through

	Decoding
	Video Output
	1×CVBS; 1×YPbPr ; 1×HDMI; 2×HD-SDI

	
	Resolution
	480i，480p，576i，576p，720p@50，720p@60，1080i@50，1080i@60, 1080p@50, 1080p@60

	
	Rate Control
	CBR/VBR  

	
	Audio Output
	1*Stereo /2*mono, HDMI，SDI

	
	Audio Sampling
	48KHz  

	
	Audio Bit Rate
	64Kbps-384Kbps  

	Stream Out
	3*IP over UDP protocol, 2*100M/1000M Base-T Ethernet Interface, one for backup

	
	2 groups separate ASI outputs (each group has 2 channels, as a copy of one of IP) output, BNC interface

	System Function 
	LCD & Key board control; web-based NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm (WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 200V-240V, 50/60Hz, 2A


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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