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FMUSER FUQ-4359 Bidirectional Transcoder 8 IP + 6 Tuner-ASI Inputs MPTS-SPTS Outputs UDP-RTP-RTSP MPEG-2 H.264 HD-SD BISS Descramble Broadcast Operators
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Product overview
The FMUSER FUQ-4359 is a bidirectional transcoder supporting H.264/MPEG-2 and HD/SD conversion, with 6 tuner inputs and ASI/IP inputs for reception, and outputs MPTS/SPTS via IP or ASI. It performs any-to-any transcoding with CBR/VBR rate control. Features include BISS descrambling, CC support, and web NMS management with LCD/keyboard interface. Ideal for satellite TV operators and broadcast content distribution. 
Key feature
Supports versatile inputs: 8×IP (SPTS/MPTS) plus 6×tuners or 6×ASI.  
Delivers flexible outputs: 8×SPTS & 1×MPTS via UDP/RTP/RTSP, plus ASI output.  
Enables advanced transcoding: Any-to-any MPEG-2/H.264 conversion in HD/SD with CBR/VBR control.  
Features integrated security: BISS descrambling and CC support.  
Provides centralized control: Web NMS management with LCD/keyboard interface.         
Principle Chart (FU-4359)
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Transcoding Mode Example
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Technical Specifications
	Stream In
	MPTS/SPTS over UDP/RTP, 1000M Base-T Ethernet Interface/ SFP interface

	
	6 * (DVB-S/S2/C/T/ISDB-T/ATSC) Tuners; 6 * ASI (optional)

	BISS Descramble
	Maximum 8 programs

	Video 
	Resolution
	1920x1080P,1920x1080i,1280x720P, 720x576i, 720x480i
480x576, 544x576, 640x576, 704x576

	
	Trans-coding
	4*MPEG2 HD → 4*MPEG2/H.264 HD ;
4*MPEG2 HD → 4*MPEG2/H.264 SD ;
8 *MPEG2 SD → 8 *MPEG2/H.264 SD

	
	
	4* H.264 HD → 4*MPEG2/H.264 HD ;
4* H.264 HD → 4*MPEG2/H.264 SD ;
8* H.264 SD → 8 *MPEG2/H.264 SD

	
	Rate Control
	CBR/VBR  

	Audio 
	Trans-coding
	MPEG-1 Layer 2, AAC and AC3(Optional) any-to-any or pass through

	
	Sampling rate
	48KHz  

	
	Bit Rate
	64Kbps-384Kbps  

	Stream Out
	8*SPTS & 1*MPTS over UDP/RTP/RTSP, 1000M Base-T Ethernet Interface (UDP/RTP uni-cast / multicast)  /SFP interface

	
	1*ASI (as a copy of one of the 8 SPTS or the MPTS) output, BNC interface

	System Function 
	LCD & Key board control; web NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm(WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 110V±10%, 50/60Hz or AC 220V±10%,50/60Hz 

	
	Power consumption  
	20W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
        
   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image4.jpeg
8 *IP (MPTS/SPTS)

6*Tuner or
6*AS|

De-Mux
&
BISS
Descrambling

Transcoding

2*SD/1*HD
2*SD/1*HD
2*SD/1*HD
2*SD/1*HD

Prog 1
Prog 2
Prog 3
Prog 4
Prog 5
Prog 6
Prog 7.
Prog 8

Re-Mux

8*SPTS &1*MPTS
ouT

ASI OUT

as a copy of 1
SPTS or MPTS




image5.jpeg
Video Transcoding

we

Passthrough

Audio Transcoding




image2.jpeg




image3.jpeg
CC (Closed Capfion)
BISS Descrambling





image1.png
FMuser




