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FUQ-4359 Transcoder 6 Tuner-ASI Inputs 8 IP Inputs DVB-S-S2-C-T-ISDB-T-ATSC to IP-ASI Outputs Bidirectional H.264-MPEG2 Transcoding BISS CC Support for Broadcast Operators
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Product overview
The FUQ-4359 transcoder performs bidirectional conversion between H.264 and MPEG-2 formats, supporting HD/SD video. It includes 6 tuner or ASI inputs and 8 IP inputs, with outputs via IP or ASI. Managed via web-based NMS, it handles signal transcoding efficiently. Ideal for broadcast operators in television and media distribution. 
Key feature
Supports bidirectional transcoding between H.264 and MPEG-2 for SD/HD programs.  
Features flexible I/O with 6 tuner/ASI inputs, 8 IP inputs, 8 SPTS and 1 MPTS over IP/ASI outputs.  
Includes BISS descrambling and closed captioning support.  
Enables remote control and monitoring via web-based NMS.        
        Principle Chart (FU-4359)
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Transcoding Mode Example
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Technical Specifications
	Stream In
	MPTS/SPTS over UDP/RTP, 1000M Base-T Ethernet Interface/ SFP interface

	
	6 * (DVB-S/S2/C/T/ISDB-T/ATSC) Tuners; 6 * ASI (optional)

	BISS Descramble
	Maximum 8 programs

	Video 
	Resolution
	1920x1080P,1920x1080i,1280x720P, 720x576i, 720x480i
480x576, 544x576, 640x576, 704x576

	
	Trans-coding
	4*MPEG2 HD → 4*MPEG2/H.264 HD ;
4*MPEG2 HD → 4*MPEG2/H.264 SD ;
8 *MPEG2 SD → 8 *MPEG2/H.264 SD

	
	
	4* H.264 HD → 4*MPEG2/H.264 HD ;
4* H.264 HD → 4*MPEG2/H.264 SD ;
8* H.264 SD → 8 *MPEG2/H.264 SD

	
	Rate Control
	CBR/VBR  

	Audio 
	Trans-coding
	MPEG-1 Layer 2, AAC and AC3(Optional) any-to-any or pass through

	
	Sampling rate
	48KHz  

	
	Bit Rate
	64Kbps-384Kbps  

	Stream Out
	8*SPTS & 1*MPTS over UDP/RTP/RTSP, 1000M Base-T Ethernet Interface (UDP/RTP uni-cast / multicast)  /SFP interface

	
	1*ASI (as a copy of one of the 8 SPTS or the MPTS) output, BNC interface

	System Function 
	LCD & Key board control; web NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm(WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 110V±10%, 50/60Hz or AC 220V±10%,50/60Hz 

	
	Power consumption  
	20W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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