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FMUSER FUQ-4359B Transcoder 4 Tuner + 8 IP Inputs MPEG-2 H.264 MPEG-2 HD SD Bidirectional Transcoding ASI UDP-RTP Streaming BISS Descrambling Cable Satellite Broadcast
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Remarks: All H.264 mentioned in this sheet refers to MPEG-4 AVC/H.264.
Product overview
The FMUSER FUQ-4359B transcoder enables bidirectional conversion between H.264 and MPEG-2, HD and SD. It processes signals with inputs including 4 tuners featuring CAM/CI slots and IP inputs, and outputs MPTS/SPTS via ASI or DATA ports. Managed via web-based NMS, it suits broadcast operators in cable TV and satellite systems for efficient signal handling. 
Key feature
Supports bidirectional video transcoding between MPEG-2 and H.264 for up to 8 SD or 4 HD programs.  
Includes flexible I/O with 4 tuners having CAM/CI slots, 8 IP inputs, and outputs via ASI or UDP/RTP/RTSP for 8 SPTS & 1 MPTS.  
Handles audio transcoding for LC-AAC, MP2, and AC3 formats with any-to-any conversion.  
Offers advanced functions like BISS descrambling, CC, and web-based NMS control.  
Principle Chart 
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Transcoding Mode Example
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Technical Specifications
	Stream In
	MPTS/SPTS over UDP/RTP, 1000M Base-T Ethernet Interface/SFP interface

	
	4 * (DVB-S/S2/C/T/ISDB-T/ATSC Optional) Tuners

	BISS Descramble
	8 programs 

	Video 
	Resolution
	1920x1080P,1920x1080i,1280x720P, 720x576i, 720x480i
480x576, 544x576, 640x576, 704x576

	
	Trans-coding
	4*MPEG2 HD → 4*MPEG2/H.264 HD ;
4*MPEG2 HD → 4*MPEG2/H.264 SD ;
8 *MPEG2 SD → 8 *MPEG2/H.264 SD

	
	
	4* H.264 HD → 4*MPEG2/H.264 HD ;
4* H.264 HD → 4*MPEG2/H.264 SD ;
8* H.264 SD → 8 *MPEG2/H.264 SD

	
	Rate Control
	CBR/VBR  

	Audio 
	Trans-coding
	MPEG-1 Layer 2, LC-AAC and AC3 any-to-any or pass through

	
	Sampling rate
	48KHz  

	
	Bit Rate
	64Kbps-384Kbps  

	Stream Out
	8*SPTS & 1*MPTS over UDP/RTP/RTSP, 1000M Base-T Ethernet Interface (UDP/RTP uni-cast / multicast)  /SFP interface

	
	1*ASI (as a copy of one of the 8 SPTS or the MPTS) output, BNC interface

	System Function 
	LCD & Key board control; web-based NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm (WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 200V-240V, 50/60Hz, 2A

	
	Power consumption  
	20W


 
Order Information
	Version
	4* ASI or Tuner Input
	6* ASI or Tuner Input
	4* Tuner input
 
	IP Input
	CAM/CI

	Simple Version (FU-4359B)
	*  
	 
	 
	 
	 

	Advanced Version (FU-4359)
	 
	*
	 
 
	          * 
	 

	FU-4359A
	 
	 
	* 
	* 
	* 


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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