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Remarks: All H.264 mentioned in this sheet refers to MPEG-4 AVC/H.264.
Product overview
The FMUSER FUQ-4359B is a bidirectional transcoder converting video between H.264 and MPEG-2 formats, including HD to SD. It supports 4 tuner inputs with CAM/CI slots and IP input, outputting MPTS and SPTS via IP or ASI. Features BISS descrambling, CC, and web-based NMS management for broadcast systems requiring flexible format conversion. 
Key feature
- Bidirectional Video Transcoding: Converts between H.264 and MPEG-2 for HD/SD resolutions.  
- Flexible I/O Configuration: Supports 8 IP inputs, 4 tuner inputs with CAM/CI, outputs 8 SPTS and 1 MPTS via IP/ASI.  
- Audio Processing: Handles LC-AAC, MP2, and AC3 with any-to-any conversion.  
- Advanced Control: Features CBR/VBR rate control, BISS descrambling, and CC.  
- Management System: Web-based NMS for monitoring and control.  
Principle Chart 
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Transcoding Mode Example
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Technical Specifications
	Stream In
	MPTS/SPTS over UDP/RTP, 1000M Base-T Ethernet Interface/SFP interface

	
	4 * (DVB-S/S2/C/T/ISDB-T/ATSC Optional) Tuners

	BISS Descramble
	8 programs 

	Video 
	Resolution
	1920x1080P,1920x1080i,1280x720P, 720x576i, 720x480i
480x576, 544x576, 640x576, 704x576

	
	Trans-coding
	4*MPEG2 HD → 4*MPEG2/H.264 HD ;
4*MPEG2 HD → 4*MPEG2/H.264 SD ;
8 *MPEG2 SD → 8 *MPEG2/H.264 SD

	
	
	4* H.264 HD → 4*MPEG2/H.264 HD ;
4* H.264 HD → 4*MPEG2/H.264 SD ;
8* H.264 SD → 8 *MPEG2/H.264 SD

	
	Rate Control
	CBR/VBR  

	Audio 
	Trans-coding
	MPEG-1 Layer 2, LC-AAC and AC3 any-to-any or pass through

	
	Sampling rate
	48KHz  

	
	Bit Rate
	64Kbps-384Kbps  

	Stream Out
	8*SPTS & 1*MPTS over UDP/RTP/RTSP, 1000M Base-T Ethernet Interface (UDP/RTP uni-cast / multicast)  /SFP interface

	
	1*ASI (as a copy of one of the 8 SPTS or the MPTS) output, BNC interface

	System Function 
	LCD & Key board control; web-based NMS management

	
	Ethernet software upgrade 

	General 
	Dimensions
	430mm×405mm×45mm (WxDxH)  

	
	Approx weight
	4.8 Kg  

	
	Temperature range 
	 0~45℃(Operation), -20~80℃(Storage) 

	
	Power requirements  
	AC 200V-240V, 50/60Hz, 2A

	
	Power consumption  
	20W


 
Order Information
	Version
	4* ASI or Tuner Input
	6* ASI or Tuner Input
	4* Tuner input
 
	IP Input
	CAM/CI

	Simple Version (FU-4359B)
	*  
	 
	 
	 
	 

	Advanced Version (FU-4359)
	 
	*
	 
 
	          * 
	 

	FU-4359A
	 
	 
	* 
	* 
	* 


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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