[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[bookmark: _GoBack]FMUSER FUQ-4412B QAM Modulator 1ch ASI Input - RF Output DVB-C ITU-T J.83A-B-C QAM Modulation TS Processing RS Encoding Broadcast Satellite Applications [image: 3EEECN_20180828012719]Product overview
The FMUSER FUQ-4412B QAM Modulator performs QAM modulation with TS and ASI inputs and RF output. It processes transport streams, applies RS encoding and convolution interlacing, and modulates signals to RF. This device supports local control via LCD/keyboard and remote NMS control. Ideal for broadcasting, interactive services, and news gathering applications.
Key feature
Enables PSI/SI processing with PID filtering, re-mapping, PCR adjustment, and NIT insertion. 
Specifications
	Input
	1channle ASI input, BNC interface, 75Ω

	    Modulation                 
	QAM Channel
	1

	
	Standard
	EN300 429/ITU-T J.83A/B/C

	
	Symbol Rate
	5.0~9.0Msps，1ksps stepping

	
	Constellation
	16、32、64、128、256QAM

	
	FEC
	RS(204, 188)

	RF Output
	Connector
	F Type, 75Ω impedance

	
	RF Range
	30~1000MHz，1kHzStepping

	
	Output Attenuation
	-16dBm~+12dBm，0.5dB Stepping

	System
	LCD/keyboard operating and NMS support

	
	English and Chinese interface conversion

	
	Ethernet software upgrading

	General
	Dimension(W*D*H)
	482mm×300mm×44mm

	
	Weight
	2.3kg

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 110V±10%，50/60Hz； or AC 220V±10%，50/60Hz

	
	Consumption
	22W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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