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The FMUSER FUQ-4412C is a QAM modulator supporting ASI and IP inputs for RF output. It processes transport streams with QAM modulation. Features include PID filtering, NIT insertion, and intelligent TS management. Ideal for broadcasting and interactive services.[image: IMG_256]
Key feature
Delivers RF output in 30–960 MHz range with 1 kHz stepping and attenuation control. 
Specifications
	Input
	1 channel ASI input, BNC interface, 75Ω

	
	1 channel IP (MPTS/SPTS) input over UDP (Unicast/Multicast) (100M Port)

	    Modulation                 
	QAM Channel
	1

	
	Standard
	EN300 429/ITU-T J.83A/B/C, GB/T170

	
	Symbol Rate
	5.0~7.0Msps，1ksps stepping

	
	Constellation
	16/32/64/128/256 QAM

	
	FEC
	RS (204, 188)

	RF Output
	Connector
	F Type, 75Ω impedance

	
	RF Range
	30~960MHz，1kHz Stepping

	
	Output Attenuation
	-30dBm~0dBm, 0.5dB Stepping

	System
	LCD/Keyboard operating and web NMS support

	
	Ethernet software upgrading

	General
	Dimension(W*D*H)
	482mm×300mm×44mm

	
	Weight
	2.3kg

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 110V±10%, 50/60Hz
or AC 220V±10%, 50/60Hz

	
	Consumption
	22W


 
 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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