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The FMUSER FUQ-4417 is an IP to ISDB-T modulator that processes 4 IP streams input and output via 1000M port, delivering multiplexed RF output. It modulates IP streams into ISDB-T signals compliant with ARIB STD-831. Control is available through web-based NMS and a front-panel LCD/keyboard. Ideal for broadcast transmission in television and radio industries.   
Key feature
- Supports ARIB STD-831 compliance for reliable broadcasting.  
- Handles 4 IP streams input/output via 1000M port.  
- Delivers multiplexed RF output with dual adjacent carriers and 30–1000MHz/1kHz tuning.  
- Features PID remapping and modulation options from DQPSK to 64QAM.  
- Offers dual control interfaces: front-panel LCD/keyboard and web-based NMS.  
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Key feature
*  Complying with ARIB STD-831 standard
*  1000M IP port, 4 IP streams input
*  Support 4 IP output
* Programs output through RF with multiplexing
*  Dual adjacent carriers output
* RF Output frequency range: 30MHz~1000MHz in 1 kHz step
*  Support PID remapping
*  LCD/keyboard and Web-based NMS operation
 
Specifications
	IP Input
	4* IP (MPTS/SPTS) input over UDP (Unitcast/Multicast) (1000M port based Ethernet)

	
	IGMP Snooping: v2, v3

	RF Output
	Standard
	ARIB STD-B31

	
	Bandwidth
	6M

	
	Constellation
	DQPSK, QPSK, 16QAM, 64QAM

	
	Guard Interval
	1/32, 1/16, 1/8, 1/4.

	
	Transmission Mode
	2K, 4K, 8K

	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	MER
	≥42dB

	
	Output
	30~1000MHz, 1KHz step

	
	RF output level
	-30~ -10dbm (77~97 dbµV), 0.1db step

	IP Output
	4*IP output, one for one with the 4 IP input

	System
	LCD/keyboard operating and Web-based NMS support

	
	Ethernet software upgrading

	General
	Dimension
	482mm×300mm×44mm (W*D*H)

	
	Weight
	2.3kg

	
	Temperature
	0~45℃(Operation); -20~80℃(Storage)

	
	Power
	AC 110V±10%, 50/60Hz; or AC 220V±10%, 50/60Hz

	
	Consumption
	25W


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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