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* 3 GE ports for IP input and output
* Support 8 (or 16) multiplexed TS over UDP/RTP/RTSP output
* 8 (or 16) non-adjacent carriers output, compliant to ISDB-Tb (ARIB STD-B31)
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* GE/SFP port alternative, with Data1 bi-directional for data in/out, and Data2-4 one-way for data in
* Supports 6 ASI input and 2 ASI output as mirror, TS file input through USB disk
* Support 8 (or 16) multiplexed TS over UDP/RTP/RTSP output
* 8 (or 16) ISDB-T non-adjacent carriers output, compliant to ARIB STD-B31 standard
 
Product Overview
The FMUSER FUQ-4417B converts IP streams into 8 or 16 non-adjacent carriers compliant with ARIB STD-B31. It performs modulation for ISDB-Tb broadcasting. Featuring web-based network management for centralized control. Ideal for DTV broadcasting systems and next-gen applications. 
Key feature
Supports 8/16 non-adjacent carriers output compliant with ISDB-Tb (ARIB STD-B31).  
Delivers 840Mbps throughput per GE input port with SFP/GE alternatives.  
Features advanced signal processing including PID remapping, PSI/SI editing, and PCR adjusting.  
Provides web-based network management for centralized control.  
Offers multi-input support with 6 ASI inputs, USB TS file ingestion, and UDP/RTP/RTSP outputs.
Inner Principle Chart
(V 1, 8ch or 16ch out for option)
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(V 2, 8ch or 16ch out for option)
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Carrier Setting Illustration:
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Specifications
	Input
	Input
	Max 512 (or 1024) IP input through 100/1000M Ethernet Port (SFP interface optional) over UDP/RTP, unicast and multicast, IGMP V2/V3, Max 840Mbps for each GE input

	
	
	[bookmark: OLE_LINK8][bookmark: OLE_LINK10]6 ASI input, BNC interface - for V2 only

	
	
	TS file input through USB disk  - for V2 only

	Mux
	Input Channel
	512 (or 1024)

	
	Output Channel
	[bookmark: OLE_LINK9]8 (or 16)

	
	Max PIDs
	256 per channel

	
	Functions
	PID remapping (auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Modulation
Parameters
	Standard
	ARIB STD-B31

	
	Bandwidth
	6M

	
	Constellation
	QPSK, 16QAM, 64QAM

	
	Guard Interval
	1/32, 1/16, 1/8, 1/4

	
	Transmission Mode
	2K, 4K, 8K

	
	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	
	MER
	≥40dB

	
	RF frequency
	50~960MHz, 1KHz step

	
	RF output level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	Output Channel
	8 (or 16) non-adjacent carriers output

	RF Output
	Interface
	1 F type port, 75Ω impedance

	
	ACLR
	-50 dBc

	TS output
	8 (or 16) IP output over UDP/RTP/RTSP, unicast/multicast 
100/1000M Ethernet Ports

	
	2 ASI output, one as mirror - for V2 only

	System
	Web-based NMS management;
LCD+Keyboard management - for V2 only

	General
	Demission
	480mm×327mm×44.5mm (WxLxH)

	
	Weight
	5.5kg

	
	Temperature
	0~45℃(operation), -20~80℃ (storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz


 
Order Guide: 
	 
	V1
	V2

	
	8ch model
	16ch model
	8ch model
	16ch model

	512 IP input to 8ch ISDB-T carriers out, 8 IP out 
	x
	 
	[bookmark: OLE_LINK11]x
	 

	1024 IP input to 16ch ISDB-T carriers out, 16 IP out 
	 
	x
	 
	x

	6 ASI input, and TS files input by USB disk
	 
	 
	x
	x

	2 ASI mirror out
	 
	 
	x
	x

	LCD+Keyboard management
	 
	 
	x
	x


 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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