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The FMUSER FUQ-4419BX is an ATSC modulator supporting up to 256 IP inputs via three GE ports and delivering 8 RF output channels. It performs multiplexing and modulation compliant with ATSC A/53, including 8VSB and RS(208,188) encoding, with web-based network management for control. Ideal for ATSC broadcasting network setup and set-top box testing.
Key feature
Supports high-capacity IP input with up to 256 streams via three GE ports  
Provides robust ATSC modulation compliant with ATSC A/53, featuring 8VSB and RS(208,188) encoding  
Enables advanced signal processing including PID remapping and PSI/SI editing  
Features web-based network management for remote control and monitoring 
Inner Principle Chart
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 Carrier Setting Illustration
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Specifications
	Input
	Input
	Max 256 IP input through 3 (front-panel Data port, Data 1 and Data 2) 100/1000M Ethernet Port (SFP interface optional). Each Data1 or Data 2 port can input max 256 IP, while front-panel Data port can input max 128 IP

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	
	Transmission Rate
	Max 840Mbps for each input channel

	Mux
	Input Channel
	256

	
	Output Channel
	8

	
	Max PIDs
	180 per channel

	
	Functions
	PID remapping(auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Modulation
Parameters
	Channel
	8

	
	Modulation Standard
	ATSC A/53

	
	Constellation
	8VSB

	
	Bandwidth
	6MHz

	
	FEC
	RS(208 188)+Trellis

	RF Output
	Interface
	F typed output port for 8 non-adjacent carriers

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20~+10dbm (for all carriers), 0.5db stepping

	
	MER
	≥ 40dB

	
	ACL
	-55 dBc

	TS output
	8 IP output over UDP/RTP/RTSP, unicast/multicast, 2 100/1000M Ethernet Ports

	System
	Web-based Network management

	General
	Demission
	420mm×440mm×44.5mm (WxLxH)

	
	Weight
	3kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz

	
	Consumption
	≤20W


 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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